(module Package_TO_SOT_THT:TO-92L_HandSolder (layer F.Cu) (tedit 5C39FB0E)
  (descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm, hand-soldering variant with enlarged pads (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
  (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
  (fp_text reference Q1 (at 1.27 -3.8) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value S8050 (at 1.27 2.79) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 1.27 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.53 1.85) (end 3.07 1.85) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.5 1.75) (end 3 1.75) (layer F.Fab) (width 0.1))
  (fp_line (start -1.46 -3.05) (end 4 -3.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.45 -3.05) (end -1.46 2.01) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4 2.01) (end 4 -3.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4 2.01) (end -1.46 2.01) (layer F.CrtYd) (width 0.05))
  (fp_arc (start 1.27 0) (end 1.27 -2.48) (angle 135) (layer F.Fab) (width 0.1))
  (fp_arc (start 1.27 0) (end 0.45 -2.45) (angle -116.9763941) (layer F.SilkS) (width 0.12))
  (fp_arc (start 1.27 0) (end 1.27 -2.48) (angle -135) (layer F.Fab) (width 0.1))
  (fp_arc (start 1.27 0) (end 2.05 -2.45) (angle 117.6433766) (layer F.SilkS) (width 0.12))
  (pad 2 thru_hole roundrect (at 1.27 -1.27) (size 1.1 1.8) (drill 0.75 (offset 0 -0.4)) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad 3 thru_hole roundrect (at 2.54 0) (size 1.1 1.8) (drill 0.75 (offset 0 0.4)) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad 1 thru_hole rect (at 0 0) (size 1.1 1.8) (drill 0.75 (offset 0 0.4)) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92L.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
