(module HASwitchPlate:ACDC-Converter_MeanWell-IRM-03-x (layer F.Cu) (tedit 5AC6543F)
  (descr "ACDC-Converter, 3W, Meanwell, IRM-03, THT")
  (fp_text reference U1 (at -15 -5) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value IRM-03-5 (at -15 19) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center -2 -2) (end -1.9 -1.9) (layer F.Fab) (width 0.1))
  (fp_line (start 3.26 -3.11) (end -33.74 -3.11) (layer F.Fab) (width 0.1))
  (fp_line (start 3.26 -3.11) (end 3.26 20.89) (layer F.Fab) (width 0.1))
  (fp_line (start -33.74 -3.11) (end -33.74 20.89) (layer F.Fab) (width 0.1))
  (fp_line (start 3.26 20.89) (end -33.74 20.89) (layer F.Fab) (width 0.1))
  (fp_line (start 3.76 21.39) (end -34.24 21.39) (layer Eco1.User) (width 0.12))
  (fp_line (start 3.76 -3.61) (end -34.24 -3.61) (layer Eco1.User) (width 0.12))
  (fp_line (start -34.24 -3.61) (end -34.24 21.39) (layer Eco1.User) (width 0.12))
  (fp_line (start 3.76 -3.61) (end 3.76 21.39) (layer Eco1.User) (width 0.12))
  (fp_line (start 4.01 21.64) (end -34.49 21.64) (layer F.CrtYd) (width 0.05))
  (fp_line (start -34.49 -3.86) (end -34.49 21.64) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.01 -3.86) (end -34.49 -3.86) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.01 -3.86) (end 4.01 21.64) (layer F.CrtYd) (width 0.05))
  (pad 4 thru_hole circle (at -30.48 17.7) (size 2.29 2.29) (drill 0.76) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -25.4 17.7) (size 2.29 2.29) (drill 0.76) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -5.08 0) (size 2.29 2.29) (drill 0.76) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 0 0) (size 2.29 2.29) (drill 0.76) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -30.48 0) (size 2.29 2.29) (drill 0.76) (layers *.Cu *.Mask))
  (model "shapes3D/Mean Well IRM-03 Series.wrl"
    (offset (xyz -33.78199949264526 3.047999954223633 0))
    (scale (xyz 0.393 0.393 0.393))
    (rotate (xyz 0 0 90))
  )
)
