diff -Naur lm_sensors-3.2.0-old/lib/sensors.conf.5 lm_sensors-3.2.0-new/lib/sensors.conf.5
--- lm_sensors-3.2.0-old/lib/sensors.conf.5	2009-02-15 09:22:38.000000000 -0800
+++ lm_sensors-3.2.0-new/lib/sensors.conf.5	2010-12-13 18:45:54.000000000 -0800
@@ -402,7 +402,7 @@
 again immediately.
 
 So, in addition to tempX_max, many chips have a tempX_max_hyst
-sub-feature. Likewise, tempX_crit often comes with tempX_max_crit.
+sub-feature. Likewise, tempX_crit often comes with tempX_crit_hyst.
 Example:
 
 .RS
