From da8a71104dda4a85a9d9546ff462542347f8efa6 Mon Sep 17 00:00:00 2001
From: Matthias Reichl <hias@horus.com>
Date: Wed, 20 Mar 2019 09:11:53 +0100
Subject: [PATCH] media: rc: rcmm decoder and encoder

commit 721074b03411327e7bf41555d4cc7c18f49313f7 upstream.

media: add support for RCMM infrared remote controls.

Signed-off-by: Patrick Lerda <patrick9876@free.fr>
Signed-off-by: Sean Young <sean@mess.org>
Signed-off-by: Mauro Carvalho Chehab <mchehab+samsung@kernel.org>
Signed-off-by: Matthias Reichl <hias@horus.com>
---
 Documentation/media/lirc.h.rst.exceptions |   3 +
 MAINTAINERS                               |   5 +
 drivers/media/rc/Kconfig                  |  13 ++
 drivers/media/rc/Makefile                 |   1 +
 drivers/media/rc/ir-rcmm-decoder.c        | 254 ++++++++++++++++++++++
 drivers/media/rc/rc-core-priv.h           |   5 +
 drivers/media/rc/rc-main.c                |   9 +
 include/media/rc-map.h                    |  14 +-
 include/uapi/linux/lirc.h                 |   6 +
 tools/include/uapi/linux/lirc.h           |  12 +
 10 files changed, 319 insertions(+), 3 deletions(-)
 create mode 100644 drivers/media/rc/ir-rcmm-decoder.c

diff --git a/Documentation/media/lirc.h.rst.exceptions b/Documentation/media/lirc.h.rst.exceptions
index 984b61dc3f2e..e7a41d4b3d46 100644
--- a/Documentation/media/lirc.h.rst.exceptions
+++ b/Documentation/media/lirc.h.rst.exceptions
@@ -58,6 +58,9 @@ ignore symbol RC_PROTO_SHARP
 ignore symbol RC_PROTO_XMP
 ignore symbol RC_PROTO_CEC
 ignore symbol RC_PROTO_IMON
+ignore symbol RC_PROTO_RCMM12
+ignore symbol RC_PROTO_RCMM24
+ignore symbol RC_PROTO_RCMM32
 
 # Undocumented macros
 
diff --git a/MAINTAINERS b/MAINTAINERS
index 9e9b19ecf6f7..57b60dd42729 100644
--- a/MAINTAINERS
+++ b/MAINTAINERS
@@ -15837,6 +15837,11 @@ M:	David Härdeman <david@hardeman.nu>
 S:	Maintained
 F:	drivers/media/rc/winbond-cir.c
 
+RCMM REMOTE CONTROLS DECODER
+M:	Patrick Lerda <patrick9876@free.fr>
+S:	Maintained
+F:	drivers/media/rc/ir-rcmm-decoder.c
+
 WINSYSTEMS EBC-C384 WATCHDOG DRIVER
 M:	William Breathitt Gray <vilhelm.gray@gmail.com>
 L:	linux-watchdog@vger.kernel.org
diff --git a/drivers/media/rc/Kconfig b/drivers/media/rc/Kconfig
index 1021c08a9ba4..8164a889011a 100644
--- a/drivers/media/rc/Kconfig
+++ b/drivers/media/rc/Kconfig
@@ -133,6 +133,19 @@ config IR_IMON_DECODER
 	   remote control and you would like to use it with a raw IR
 	   receiver, or if you wish to use an encoder to transmit this IR.
 
+config IR_RCMM_DECODER
+	tristate "Enable IR raw decoder for the RC-MM protocol"
+	depends on RC_CORE
+	help
+	   Enable this option when you have IR with RC-MM protocol, and
+	   you need the software decoder. The driver supports 12,
+	   24 and 32 bits RC-MM variants. You can enable or disable the
+	   different modes using the following RC protocol keywords:
+	   'rc-mm-12', 'rc-mm-24' and 'rc-mm-32'.
+
+	   To compile this driver as a module, choose M here: the module
+	   will be called ir-rcmm-decoder.
+
 endif #RC_DECODERS
 
 menuconfig RC_DEVICES
diff --git a/drivers/media/rc/Makefile b/drivers/media/rc/Makefile
index e0340d043fe8..fc4058013234 100644
--- a/drivers/media/rc/Makefile
+++ b/drivers/media/rc/Makefile
@@ -16,6 +16,7 @@ obj-$(CONFIG_IR_SHARP_DECODER) += ir-sharp-decoder.o
 obj-$(CONFIG_IR_MCE_KBD_DECODER) += ir-mce_kbd-decoder.o
 obj-$(CONFIG_IR_XMP_DECODER) += ir-xmp-decoder.o
 obj-$(CONFIG_IR_IMON_DECODER) += ir-imon-decoder.o
+obj-$(CONFIG_IR_RCMM_DECODER) += ir-rcmm-decoder.o
 
 # stand-alone IR receivers/transmitters
 obj-$(CONFIG_RC_ATI_REMOTE) += ati_remote.o
diff --git a/drivers/media/rc/ir-rcmm-decoder.c b/drivers/media/rc/ir-rcmm-decoder.c
new file mode 100644
index 000000000000..f1096ac1e5c5
--- /dev/null
+++ b/drivers/media/rc/ir-rcmm-decoder.c
@@ -0,0 +1,254 @@
+// SPDX-License-Identifier: GPL-2.0+
+// ir-rcmm-decoder.c - A decoder for the RCMM IR protocol
+//
+// Copyright (C) 2018 by Patrick Lerda <patrick9876@free.fr>
+
+#include "rc-core-priv.h"
+#include <linux/module.h>
+#include <linux/version.h>
+
+#define RCMM_UNIT		166667	/* nanosecs */
+#define RCMM_PREFIX_PULSE	416666  /* 166666.666666666*2.5 */
+#define RCMM_PULSE_0            277777  /* 166666.666666666*(1+2/3) */
+#define RCMM_PULSE_1            444444  /* 166666.666666666*(2+2/3) */
+#define RCMM_PULSE_2            611111  /* 166666.666666666*(3+2/3) */
+#define RCMM_PULSE_3            777778  /* 166666.666666666*(4+2/3) */
+
+enum rcmm_state {
+	STATE_INACTIVE,
+	STATE_LOW,
+	STATE_BUMP,
+	STATE_VALUE,
+	STATE_FINISHED,
+};
+
+static bool rcmm_mode(const struct rcmm_dec *data)
+{
+	return !((0x000c0000 & data->bits) == 0x000c0000);
+}
+
+static int rcmm_miscmode(struct rc_dev *dev, struct rcmm_dec *data)
+{
+	switch (data->count) {
+	case 24:
+		if (dev->enabled_protocols & RC_PROTO_BIT_RCMM24) {
+			rc_keydown(dev, RC_PROTO_RCMM24, data->bits, 0);
+			data->state = STATE_INACTIVE;
+			return 0;
+		}
+		return -1;
+
+	case 12:
+		if (dev->enabled_protocols & RC_PROTO_BIT_RCMM12) {
+			rc_keydown(dev, RC_PROTO_RCMM12, data->bits, 0);
+			data->state = STATE_INACTIVE;
+			return 0;
+		}
+		return -1;
+	}
+
+	return -1;
+}
+
+/**
+ * ir_rcmm_decode() - Decode one RCMM pulse or space
+ * @dev:	the struct rc_dev descriptor of the device
+ * @ev:		the struct ir_raw_event descriptor of the pulse/space
+ *
+ * This function returns -EINVAL if the pulse violates the state machine
+ */
+static int ir_rcmm_decode(struct rc_dev *dev, struct ir_raw_event ev)
+{
+	struct rcmm_dec *data = &dev->raw->rcmm;
+	u32 scancode;
+	u8 toggle;
+	int value;
+
+	if (!(dev->enabled_protocols & (RC_PROTO_BIT_RCMM32 |
+							RC_PROTO_BIT_RCMM24 |
+							RC_PROTO_BIT_RCMM12)))
+		return 0;
+
+	if (!is_timing_event(ev)) {
+		if (ev.reset)
+			data->state = STATE_INACTIVE;
+		return 0;
+	}
+
+	switch (data->state) {
+	case STATE_INACTIVE:
+		if (!ev.pulse)
+			break;
+
+		if (!eq_margin(ev.duration, RCMM_PREFIX_PULSE, RCMM_UNIT / 2))
+			break;
+
+		data->state = STATE_LOW;
+		data->count = 0;
+		data->bits  = 0;
+		return 0;
+
+	case STATE_LOW:
+		if (ev.pulse)
+			break;
+
+		if (!eq_margin(ev.duration, RCMM_PULSE_0, RCMM_UNIT / 2))
+			break;
+
+		data->state = STATE_BUMP;
+		return 0;
+
+	case STATE_BUMP:
+		if (!ev.pulse)
+			break;
+
+		if (!eq_margin(ev.duration, RCMM_UNIT, RCMM_UNIT / 2))
+			break;
+
+		data->state = STATE_VALUE;
+		return 0;
+
+	case STATE_VALUE:
+		if (ev.pulse)
+			break;
+
+		if (eq_margin(ev.duration, RCMM_PULSE_0, RCMM_UNIT / 2))
+			value = 0;
+		else if (eq_margin(ev.duration, RCMM_PULSE_1, RCMM_UNIT / 2))
+			value = 1;
+		else if (eq_margin(ev.duration, RCMM_PULSE_2, RCMM_UNIT / 2))
+			value = 2;
+		else if (eq_margin(ev.duration, RCMM_PULSE_3, RCMM_UNIT / 2))
+			value = 3;
+		else
+			value = -1;
+
+		if (value == -1) {
+			if (!rcmm_miscmode(dev, data))
+				return 0;
+			break;
+		}
+
+		data->bits <<= 2;
+		data->bits |= value;
+
+		data->count += 2;
+
+		if (data->count < 32)
+			data->state = STATE_BUMP;
+		else
+			data->state = STATE_FINISHED;
+
+		return 0;
+
+	case STATE_FINISHED:
+		if (!ev.pulse)
+			break;
+
+		if (!eq_margin(ev.duration, RCMM_UNIT, RCMM_UNIT / 2))
+			break;
+
+		if (rcmm_mode(data)) {
+			toggle = !!(0x8000 & data->bits);
+			scancode = data->bits & ~0x8000;
+		} else {
+			toggle = 0;
+			scancode = data->bits;
+		}
+
+		if (dev->enabled_protocols & RC_PROTO_BIT_RCMM32) {
+			rc_keydown(dev, RC_PROTO_RCMM32, scancode, toggle);
+			data->state = STATE_INACTIVE;
+			return 0;
+		}
+
+		break;
+	}
+
+	data->state = STATE_INACTIVE;
+	return -EINVAL;
+}
+
+static const int rcmmspace[] = {
+	RCMM_PULSE_0,
+	RCMM_PULSE_1,
+	RCMM_PULSE_2,
+	RCMM_PULSE_3,
+};
+
+static int ir_rcmm_rawencoder(struct ir_raw_event **ev, unsigned int max,
+			      unsigned int n, u32 data)
+{
+	int i;
+	int ret;
+
+	ret = ir_raw_gen_pulse_space(ev, &max, RCMM_PREFIX_PULSE, RCMM_PULSE_0);
+	if (ret)
+		return ret;
+
+	for (i = n - 2; i >= 0; i -= 2) {
+		const unsigned int space = rcmmspace[(data >> i) & 3];
+
+		ret = ir_raw_gen_pulse_space(ev, &max, RCMM_UNIT, space);
+		if (ret)
+			return ret;
+	}
+
+	return ir_raw_gen_pulse_space(ev, &max, RCMM_UNIT, RCMM_PULSE_3 * 2);
+}
+
+static int ir_rcmm_encode(enum rc_proto protocol, u32 scancode,
+			  struct ir_raw_event *events, unsigned int max)
+{
+	struct ir_raw_event *e = events;
+	int ret;
+
+	switch (protocol) {
+	case RC_PROTO_RCMM32:
+		ret = ir_rcmm_rawencoder(&e, max, 32, scancode);
+		break;
+	case RC_PROTO_RCMM24:
+		ret = ir_rcmm_rawencoder(&e, max, 24, scancode);
+		break;
+	case RC_PROTO_RCMM12:
+		ret = ir_rcmm_rawencoder(&e, max, 12, scancode);
+		break;
+	default:
+		ret = -EINVAL;
+	}
+
+	if (ret < 0)
+		return ret;
+
+	return e - events;
+}
+
+static struct ir_raw_handler rcmm_handler = {
+	.protocols	= RC_PROTO_BIT_RCMM32 |
+			  RC_PROTO_BIT_RCMM24 |
+			  RC_PROTO_BIT_RCMM12,
+	.decode		= ir_rcmm_decode,
+	.encode         = ir_rcmm_encode,
+	.carrier        = 36000,
+	.min_timeout	= RCMM_PULSE_3 + RCMM_UNIT,
+};
+
+static int __init ir_rcmm_decode_init(void)
+{
+	ir_raw_handler_register(&rcmm_handler);
+
+	pr_info("IR RCMM protocol handler initialized\n");
+	return 0;
+}
+
+static void __exit ir_rcmm_decode_exit(void)
+{
+	ir_raw_handler_unregister(&rcmm_handler);
+}
+
+module_init(ir_rcmm_decode_init);
+module_exit(ir_rcmm_decode_exit);
+
+MODULE_LICENSE("GPL");
+MODULE_AUTHOR("Patrick Lerda");
+MODULE_DESCRIPTION("RCMM IR protocol decoder");
diff --git a/drivers/media/rc/rc-core-priv.h b/drivers/media/rc/rc-core-priv.h
index e847bdad5c51..59c252f24194 100644
--- a/drivers/media/rc/rc-core-priv.h
+++ b/drivers/media/rc/rc-core-priv.h
@@ -136,6 +136,11 @@ struct ir_raw_event_ctrl {
 		struct input_dev *idev;
 		char name[64];
 	} imon;
+	struct rcmm_dec {
+		int state;
+		unsigned int count;
+		u32 bits;
+	} rcmm;
 };
 
 /* Mutex for locking raw IR processing and handler change */
diff --git a/drivers/media/rc/rc-main.c b/drivers/media/rc/rc-main.c
index 0f218afdadaa..78e79c37f208 100644
--- a/drivers/media/rc/rc-main.c
+++ b/drivers/media/rc/rc-main.c
@@ -70,6 +70,12 @@ static const struct {
 	[RC_PROTO_CEC] = { .name = "cec", .repeat_period = 0 },
 	[RC_PROTO_IMON] = { .name = "imon",
 		.scancode_bits = 0x7fffffff, .repeat_period = 114 },
+	[RC_PROTO_RCMM12] = { .name = "rc-mm-12",
+		.scancode_bits = 0x00000fff, .repeat_period = 114 },
+	[RC_PROTO_RCMM24] = { .name = "rc-mm-24",
+		.scancode_bits = 0x00ffffff, .repeat_period = 114 },
+	[RC_PROTO_RCMM32] = { .name = "rc-mm-32",
+		.scancode_bits = 0xffffffff, .repeat_period = 114 },
 };
 
 /* Used to keep track of known keymaps */
@@ -1018,6 +1024,9 @@ static const struct {
 	{ RC_PROTO_BIT_XMP,	"xmp",		"ir-xmp-decoder"	},
 	{ RC_PROTO_BIT_CEC,	"cec",		NULL			},
 	{ RC_PROTO_BIT_IMON,	"imon",		"ir-imon-decoder"	},
+	{ RC_PROTO_BIT_RCMM12 |
+	  RC_PROTO_BIT_RCMM24 |
+	  RC_PROTO_BIT_RCMM32,	"rc-mm",	"ir-rcmm-decoder"	},
 };
 
 /**
diff --git a/include/media/rc-map.h b/include/media/rc-map.h
index bfa3017cecba..cf308b73edae 100644
--- a/include/media/rc-map.h
+++ b/include/media/rc-map.h
@@ -37,6 +37,9 @@
 #define RC_PROTO_BIT_XMP		BIT_ULL(RC_PROTO_XMP)
 #define RC_PROTO_BIT_CEC		BIT_ULL(RC_PROTO_CEC)
 #define RC_PROTO_BIT_IMON		BIT_ULL(RC_PROTO_IMON)
+#define RC_PROTO_BIT_RCMM12		BIT_ULL(RC_PROTO_RCMM12)
+#define RC_PROTO_BIT_RCMM24		BIT_ULL(RC_PROTO_RCMM24)
+#define RC_PROTO_BIT_RCMM32		BIT_ULL(RC_PROTO_RCMM32)
 
 #define RC_PROTO_BIT_ALL \
 			(RC_PROTO_BIT_UNKNOWN | RC_PROTO_BIT_OTHER | \
@@ -51,7 +54,8 @@
 			 RC_PROTO_BIT_RC6_6A_24 | RC_PROTO_BIT_RC6_6A_32 | \
 			 RC_PROTO_BIT_RC6_MCE | RC_PROTO_BIT_SHARP | \
 			 RC_PROTO_BIT_XMP | RC_PROTO_BIT_CEC | \
-			 RC_PROTO_BIT_IMON)
+			 RC_PROTO_BIT_IMON | RC_PROTO_BIT_RCMM12 | \
+			 RC_PROTO_BIT_RCMM24 | RC_PROTO_BIT_RCMM32)
 /* All rc protocols for which we have decoders */
 #define RC_PROTO_BIT_ALL_IR_DECODER \
 			(RC_PROTO_BIT_RC5 | RC_PROTO_BIT_RC5X_20 | \
@@ -64,7 +68,9 @@
 			 RC_PROTO_BIT_RC6_0 | RC_PROTO_BIT_RC6_6A_20 | \
 			 RC_PROTO_BIT_RC6_6A_24 |  RC_PROTO_BIT_RC6_6A_32 | \
 			 RC_PROTO_BIT_RC6_MCE | RC_PROTO_BIT_SHARP | \
-			 RC_PROTO_BIT_XMP | RC_PROTO_BIT_IMON)
+			 RC_PROTO_BIT_XMP | RC_PROTO_BIT_IMON | \
+			 RC_PROTO_BIT_RCMM12 | RC_PROTO_BIT_RCMM24 | \
+			 RC_PROTO_BIT_RCMM32)
 
 #define RC_PROTO_BIT_ALL_IR_ENCODER \
 			(RC_PROTO_BIT_RC5 | RC_PROTO_BIT_RC5X_20 | \
@@ -77,7 +83,9 @@
 			 RC_PROTO_BIT_RC6_0 | RC_PROTO_BIT_RC6_6A_20 | \
 			 RC_PROTO_BIT_RC6_6A_24 | \
 			 RC_PROTO_BIT_RC6_6A_32 | RC_PROTO_BIT_RC6_MCE | \
-			 RC_PROTO_BIT_SHARP | RC_PROTO_BIT_IMON)
+			 RC_PROTO_BIT_SHARP | RC_PROTO_BIT_IMON | \
+			 RC_PROTO_BIT_RCMM12 | RC_PROTO_BIT_RCMM24 | \
+			 RC_PROTO_BIT_RCMM32)
 
 #define RC_SCANCODE_UNKNOWN(x)			(x)
 #define RC_SCANCODE_OTHER(x)			(x)
diff --git a/include/uapi/linux/lirc.h b/include/uapi/linux/lirc.h
index 6b319581882f..45fcbf99d72e 100644
--- a/include/uapi/linux/lirc.h
+++ b/include/uapi/linux/lirc.h
@@ -192,6 +192,9 @@ struct lirc_scancode {
  * @RC_PROTO_XMP: XMP protocol
  * @RC_PROTO_CEC: CEC protocol
  * @RC_PROTO_IMON: iMon Pad protocol
+ * @RC_PROTO_RCMM12: RC-MM protocol 12 bits
+ * @RC_PROTO_RCMM24: RC-MM protocol 24 bits
+ * @RC_PROTO_RCMM32: RC-MM protocol 32 bits
  */
 enum rc_proto {
 	RC_PROTO_UNKNOWN	= 0,
@@ -218,6 +221,9 @@ enum rc_proto {
 	RC_PROTO_XMP		= 21,
 	RC_PROTO_CEC		= 22,
 	RC_PROTO_IMON		= 23,
+	RC_PROTO_RCMM12		= 24,
+	RC_PROTO_RCMM24		= 25,
+	RC_PROTO_RCMM32		= 26,
 };
 
 #endif
diff --git a/tools/include/uapi/linux/lirc.h b/tools/include/uapi/linux/lirc.h
index f189931042a7..45fcbf99d72e 100644
--- a/tools/include/uapi/linux/lirc.h
+++ b/tools/include/uapi/linux/lirc.h
@@ -133,6 +133,12 @@
 
 #define LIRC_SET_WIDEBAND_RECEIVER     _IOW('i', 0x00000023, __u32)
 
+/*
+ * Return the recording timeout, which is either set by
+ * the ioctl LIRC_SET_REC_TIMEOUT or by the kernel after setting the protocols.
+ */
+#define LIRC_GET_REC_TIMEOUT	       _IOR('i', 0x00000024, __u32)
+
 /*
  * struct lirc_scancode - decoded scancode with protocol for use with
  *	LIRC_MODE_SCANCODE
@@ -186,6 +192,9 @@ struct lirc_scancode {
  * @RC_PROTO_XMP: XMP protocol
  * @RC_PROTO_CEC: CEC protocol
  * @RC_PROTO_IMON: iMon Pad protocol
+ * @RC_PROTO_RCMM12: RC-MM protocol 12 bits
+ * @RC_PROTO_RCMM24: RC-MM protocol 24 bits
+ * @RC_PROTO_RCMM32: RC-MM protocol 32 bits
  */
 enum rc_proto {
 	RC_PROTO_UNKNOWN	= 0,
@@ -212,6 +221,9 @@ enum rc_proto {
 	RC_PROTO_XMP		= 21,
 	RC_PROTO_CEC		= 22,
 	RC_PROTO_IMON		= 23,
+	RC_PROTO_RCMM12		= 24,
+	RC_PROTO_RCMM24		= 25,
+	RC_PROTO_RCMM32		= 26,
 };
 
 #endif
-- 
2.20.1

