diff --git a/arch/arm/dts/sun50i-h6-pine-h64.dts b/arch/arm/dts/sun50i-h6-pine-h64.dts
index ceffc40810..bdb8470fc8 100644
--- a/arch/arm/dts/sun50i-h6-pine-h64.dts
+++ b/arch/arm/dts/sun50i-h6-pine-h64.dts
@@ -14,6 +14,7 @@
 	compatible = "pine64,pine-h64", "allwinner,sun50i-h6";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 	};
 
@@ -21,6 +22,17 @@
 		stdout-path = "serial0:115200n8";
 	};
 
+	connector {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
 	leds {
 		compatible = "gpio-leds";
 
@@ -39,6 +51,56 @@
 			gpios = <&r_pio 0 7 GPIO_ACTIVE_HIGH>; /* PL7 */
 		};
 	};
+
+	reg_usb_vbus: vbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usb-vbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		startup-delay-us = <100000>;
+		gpio = <&r_pio 0 5 GPIO_ACTIVE_HIGH>;
+		enable-active-high;
+	};
+};
+
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&ext_rgmii_pins>;
+	phy-mode = "rgmii";
+	phy-handle = <&ext_rgmii_phy>;
+	phy-supply = <&reg_aldo2>;
+	allwinner,rx-delay-ps = <200>;
+	allwinner,tx-delay-ps = <200>;
+	status = "okay";
+};
+
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
+&de {
+	status = "okay";
+};
+
+&hdmi {
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&ehci3 {
+	status = "okay";
 };
 
 &mmc0 {
@@ -46,6 +108,7 @@
 	pinctrl-0 = <&mmc0_pins>;
 	vmmc-supply = <&reg_cldo1>;
 	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>;
+	bus-width = <4>;
 	status = "okay";
 };
 
@@ -56,6 +119,15 @@
 	vqmmc-supply = <&reg_bldo2>;
 	non-removable;
 	cap-mmc-hw-reset;
+	bus-width = <8>;
+	status = "okay";
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&ohci3 {
 	status = "okay";
 };
 
@@ -83,6 +155,7 @@
 				regulator-min-microvolt = <3300000>;
 				regulator-max-microvolt = <3300000>;
 				regulator-name = "vcc-ac200";
+				regulator-enable-ramp-delay = <100000>;
 			};
 
 			reg_aldo3: aldo3 {
@@ -183,3 +256,14 @@
 	pinctrl-0 = <&uart0_ph_pins>;
 	status = "okay";
 };
+
+&usb2otg {
+	dr_mode = "host";
+	status = "okay";
+};
+
+&usb2phy {
+	usb0_vbus-supply = <&reg_usb_vbus>;
+	usb3_vbus-supply = <&reg_usb_vbus>;
+	status = "okay";
+};
diff --git a/arch/arm/dts/sun50i-h6.dtsi b/arch/arm/dts/sun50i-h6.dtsi
index cfa5fffcf6..c9e861a50a 100644
--- a/arch/arm/dts/sun50i-h6.dtsi
+++ b/arch/arm/dts/sun50i-h6.dtsi
@@ -6,8 +6,11 @@
 #include <dt-bindings/interrupt-controller/arm-gic.h>
 #include <dt-bindings/clock/sun50i-h6-ccu.h>
 #include <dt-bindings/clock/sun50i-h6-r-ccu.h>
+#include <dt-bindings/clock/sun8i-de2.h>
+#include <dt-bindings/clock/sun8i-tcon-top.h>
 #include <dt-bindings/reset/sun50i-h6-ccu.h>
 #include <dt-bindings/reset/sun50i-h6-r-ccu.h>
+#include <dt-bindings/reset/sun8i-de2.h>
 
 / {
 	interrupt-parent = <&gic>;
@@ -19,34 +22,40 @@
 		#size-cells = <0>;
 
 		cpu0: cpu@0 {
-			compatible = "arm,cortex-a53", "arm,armv8";
+			compatible = "arm,cortex-a53";
 			device_type = "cpu";
 			reg = <0>;
 			enable-method = "psci";
 		};
 
 		cpu1: cpu@1 {
-			compatible = "arm,cortex-a53", "arm,armv8";
+			compatible = "arm,cortex-a53";
 			device_type = "cpu";
 			reg = <1>;
 			enable-method = "psci";
 		};
 
 		cpu2: cpu@2 {
-			compatible = "arm,cortex-a53", "arm,armv8";
+			compatible = "arm,cortex-a53";
 			device_type = "cpu";
 			reg = <2>;
 			enable-method = "psci";
 		};
 
 		cpu3: cpu@3 {
-			compatible = "arm,cortex-a53", "arm,armv8";
+			compatible = "arm,cortex-a53";
 			device_type = "cpu";
 			reg = <3>;
 			enable-method = "psci";
 		};
 	};
 
+	de: display-engine {
+		compatible = "allwinner,sun50i-h6-display-engine";
+		allwinner,pipelines = <&mixer0>;
+		status = "disabled";
+	};
+
 	iosc: internal-osc-clk {
 		#clock-cells = <0>;
 		compatible = "fixed-clock";
@@ -92,6 +101,88 @@
 		#size-cells = <1>;
 		ranges;
 
+		display-engine@1000000 {
+			compatible = "allwinner,sun50i-h6-de3",
+				     "allwinner,sun50i-a64-de2";
+			reg = <0x1000000 0x400000>;
+			allwinner,sram = <&de2_sram 1>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges = <0 0x1000000 0x400000>;
+
+			display_clocks: clock@0 {
+				compatible = "allwinner,sun50i-h6-de3-clk";
+				reg = <0x0 0x10000>;
+				clocks = <&ccu CLK_DE>,
+					 <&ccu CLK_BUS_DE>;
+				clock-names = "mod",
+					      "bus";
+				resets = <&ccu RST_BUS_DE>;
+				#clock-cells = <1>;
+				#reset-cells = <1>;
+			};
+
+			mixer0: mixer@100000 {
+				compatible = "allwinner,sun50i-h6-de3-mixer-0";
+				reg = <0x100000 0x100000>;
+				clocks = <&display_clocks CLK_BUS_MIXER0>,
+					 <&display_clocks CLK_MIXER0>;
+				clock-names = "bus",
+					      "mod";
+				resets = <&display_clocks RST_MIXER0>;
+
+				ports {
+					#address-cells = <1>;
+					#size-cells = <0>;
+
+					mixer0_out: port@1 {
+						reg = <1>;
+
+						mixer0_out_tcon_top_mixer0: endpoint {
+							remote-endpoint = <&tcon_top_mixer0_in_mixer0>;
+						};
+					};
+				};
+			};
+		};
+
+		syscon: syscon@3000000 {
+			compatible = "allwinner,sun50i-h6-system-control",
+				     "allwinner,sun50i-a64-system-control";
+			reg = <0x03000000 0x1000>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges;
+
+			sram_c: sram@28000 {
+				compatible = "mmio-sram";
+				reg = <0x00028000 0x1e000>;
+				#address-cells = <1>;
+				#size-cells = <1>;
+				ranges = <0 0x00028000 0x1e000>;
+
+				de2_sram: sram-section@0 {
+					compatible = "allwinner,sun50i-h6-sram-c",
+						     "allwinner,sun50i-a64-sram-c";
+					reg = <0x0000 0x1e000>;
+				};
+			};
+
+			sram_c1: sram@1a00000 {
+				compatible = "mmio-sram";
+				reg = <0x01a00000 0x200000>;
+				#address-cells = <1>;
+				#size-cells = <1>;
+				ranges = <0 0x01a00000 0x200000>;
+
+				ve_sram: sram-section@0 {
+					compatible = "allwinner,sun50i-h6-sram-c1",
+						     "allwinner,sun4i-a10-sram-c1";
+					reg = <0x000000 0x200000>;
+				};
+			};
+		};
+
 		ccu: clock@3001000 {
 			compatible = "allwinner,sun50i-h6-ccu";
 			reg = <0x03001000 0x1000>;
@@ -101,17 +192,6 @@
 			#reset-cells = <1>;
 		};
 
-		gic: interrupt-controller@3021000 {
-			compatible = "arm,gic-400";
-			reg = <0x03021000 0x1000>,
-			      <0x03022000 0x2000>,
-			      <0x03024000 0x2000>,
-			      <0x03026000 0x2000>;
-			interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
-			interrupt-controller;
-			#interrupt-cells = <3>;
-		};
-
 		pio: pinctrl@300b000 {
 			compatible = "allwinner,sun50i-h6-pinctrl";
 			reg = <0x0300b000 0x400>;
@@ -126,6 +206,19 @@
 			interrupt-controller;
 			#interrupt-cells = <3>;
 
+			ext_rgmii_pins: rgmii_pins {
+				pins = "PD0", "PD1", "PD2", "PD3", "PD4",
+				       "PD5", "PD7", "PD8", "PD9", "PD10",
+				       "PD11", "PD12", "PD13", "PD19", "PD20";
+				function = "emac";
+				drive-strength = <40>;
+			};
+
+			hdmi_pins: hdmi-pins {
+				pins = "PH8", "PH9", "PH10";
+				function = "hdmi";
+			};
+
 			mmc0_pins: mmc0-pins {
 				pins = "PF0", "PF1", "PF2", "PF3",
 				       "PF4", "PF5";
@@ -149,6 +242,17 @@
 			};
 		};
 
+		gic: interrupt-controller@3021000 {
+			compatible = "arm,gic-400";
+			reg = <0x03021000 0x1000>,
+			      <0x03022000 0x2000>,
+			      <0x03024000 0x2000>,
+			      <0x03026000 0x2000>;
+			interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
+			interrupt-controller;
+			#interrupt-cells = <3>;
+		};
+
 		mmc0: mmc@4020000 {
 			compatible = "allwinner,sun50i-h6-mmc",
 				     "allwinner,sun50i-a64-mmc";
@@ -235,6 +339,250 @@
 			status = "disabled";
 		};
 
+		emac: ethernet@5020000 {
+			compatible = "allwinner,sun50i-h6-emac",
+				     "allwinner,sun50i-a64-emac";
+			syscon = <&syscon>;
+			reg = <0x05020000 0x10000>;
+			interrupts = <GIC_SPI 12 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "macirq";
+			resets = <&ccu RST_BUS_EMAC>;
+			reset-names = "stmmaceth";
+			clocks = <&ccu CLK_BUS_EMAC>;
+			clock-names = "stmmaceth";
+			status = "disabled";
+
+			mdio: mdio {
+				compatible = "snps,dwmac-mdio";
+				#address-cells = <1>;
+				#size-cells = <0>;
+			};
+		};
+
+		usb2otg: usb@5100000 {
+			compatible = "allwinner,sun50i-h6-musb",
+				     "allwinner,sun8i-a33-musb";
+			reg = <0x05100000 0x0400>;
+			clocks = <&ccu CLK_BUS_OTG>;
+			resets = <&ccu RST_BUS_OTG>;
+			interrupts = <GIC_SPI 23 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "mc";
+			phys = <&usb2phy 0>;
+			phy-names = "usb";
+			extcon = <&usb2phy 0>;
+			status = "disabled";
+		};
+
+		usb2phy: phy@5100400 {
+			compatible = "allwinner,sun50i-h6-usb-phy";
+			reg = <0x05100400 0x24>,
+			      <0x05101800 0x4>,
+			      <0x05311800 0x4>;
+			reg-names = "phy_ctrl",
+				    "pmu0",
+				    "pmu3";
+			clocks = <&ccu CLK_USB_PHY0>,
+				 <&ccu CLK_USB_PHY3>;
+			clock-names = "usb0_phy",
+				      "usb3_phy";
+			resets = <&ccu RST_USB_PHY0>,
+				 <&ccu RST_USB_PHY3>;
+			reset-names = "usb0_reset",
+				      "usb3_reset";
+			status = "disabled";
+			#phy-cells = <1>;
+		};
+
+		ehci0: usb@5101000 {
+			compatible = "allwinner,sun50i-h6-ehci", "generic-ehci";
+			reg = <0x05101000 0x100>;
+			interrupts = <GIC_SPI 24 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI0>,
+				 <&ccu CLK_BUS_EHCI0>,
+				 <&ccu CLK_USB_OHCI0>;
+			resets = <&ccu RST_BUS_OHCI0>,
+				 <&ccu RST_BUS_EHCI0>;
+			status = "disabled";
+		};
+
+		ohci0: usb@5101400 {
+			compatible = "allwinner,sun50i-h6-ohci", "generic-ohci";
+			reg = <0x05101400 0x100>;
+			interrupts = <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI0>,
+				 <&ccu CLK_USB_OHCI0>;
+			resets = <&ccu RST_BUS_OHCI0>;
+			status = "disabled";
+		};
+
+		ehci3: usb@5311000 {
+			compatible = "allwinner,sun50i-h6-ehci", "generic-ehci";
+			reg = <0x05311000 0x100>;
+			interrupts = <GIC_SPI 28 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI3>,
+				 <&ccu CLK_BUS_EHCI3>,
+				 <&ccu CLK_USB_OHCI3>;
+			resets = <&ccu RST_BUS_OHCI3>,
+				 <&ccu RST_BUS_EHCI3>;
+			phys = <&usb2phy 3>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		ohci3: usb@5311400 {
+			compatible = "allwinner,sun50i-h6-ohci", "generic-ohci";
+			reg = <0x05311400 0x100>;
+			interrupts = <GIC_SPI 29 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI3>,
+				 <&ccu CLK_USB_OHCI3>;
+			resets = <&ccu RST_BUS_OHCI3>;
+			phys = <&usb2phy 3>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		hdmi: hdmi@6000000 {
+			compatible = "allwinner,sun50i-h6-dw-hdmi";
+			reg = <0x06000000 0x10000>;
+			reg-io-width = <1>;
+			interrupts = <GIC_SPI 64 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_HDMI>, <&ccu CLK_HDMI_SLOW>,
+				 <&ccu CLK_HDMI>, <&ccu CLK_HDMI_CEC>,
+				 <&ccu CLK_HDCP>, <&ccu CLK_BUS_HDCP>;
+			clock-names = "iahb", "isfr", "tmds", "cec", "hdcp",
+				      "hdcp-bus";
+			resets = <&ccu RST_BUS_HDMI_SUB>, <&ccu RST_BUS_HDCP>;
+			reset-names = "ctrl", "hdcp";
+			phys = <&hdmi_phy>;
+			phy-names = "hdmi-phy";
+			pinctrl-names = "default";
+			pinctrl-0 = <&hdmi_pins>;
+			status = "disabled";
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				hdmi_in: port@0 {
+					reg = <0>;
+
+					hdmi_in_tcon_top: endpoint {
+						remote-endpoint = <&tcon_top_hdmi_out_hdmi>;
+					};
+				};
+
+				hdmi_out: port@1 {
+					reg = <1>;
+				};
+			};
+		};
+
+		hdmi_phy: hdmi-phy@6010000 {
+			compatible = "allwinner,sun50i-h6-hdmi-phy";
+			reg = <0x06010000 0x10000>;
+			clocks = <&ccu CLK_BUS_HDMI>, <&ccu CLK_HDMI_SLOW>;
+			clock-names = "bus", "mod";
+			resets = <&ccu RST_BUS_HDMI>;
+			reset-names = "phy";
+			#phy-cells = <0>;
+		};
+
+		tcon_top: tcon-top@6510000 {
+			compatible = "allwinner,sun50i-h6-tcon-top";
+			reg = <0x06510000 0x1000>;
+			clocks = <&ccu CLK_BUS_TCON_TOP>,
+				 <&ccu CLK_TCON_TV0>;
+			clock-names = "bus",
+				      "tcon-tv0";
+			clock-output-names = "tcon-top-tv0";
+			resets = <&ccu RST_BUS_TCON_TOP>;
+			reset-names = "rst";
+			#clock-cells = <1>;
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				tcon_top_mixer0_in: port@0 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <0>;
+
+					tcon_top_mixer0_in_mixer0: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&mixer0_out_tcon_top_mixer0>;
+					};
+				};
+
+				tcon_top_mixer0_out: port@1 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <1>;
+
+					tcon_top_mixer0_out_tcon_tv: endpoint@2 {
+						reg = <2>;
+						remote-endpoint = <&tcon_tv_in_tcon_top_mixer0>;
+					};
+				};
+
+				tcon_top_hdmi_in: port@4 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <4>;
+
+					tcon_top_hdmi_in_tcon_tv: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&tcon_tv_out_tcon_top>;
+					};
+				};
+
+				tcon_top_hdmi_out: port@5 {
+					reg = <5>;
+
+					tcon_top_hdmi_out_hdmi: endpoint {
+						remote-endpoint = <&hdmi_in_tcon_top>;
+					};
+				};
+			};
+		};
+
+		tcon_tv: lcd-controller@6515000 {
+			compatible = "allwinner,sun50i-h6-tcon-tv",
+				     "allwinner,sun8i-r40-tcon-tv";
+			reg = <0x06515000 0x1000>;
+			interrupts = <GIC_SPI 66 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_TCON_TV0>,
+				 <&tcon_top CLK_TCON_TOP_TV0>;
+			clock-names = "ahb",
+				      "tcon-ch1";
+			resets = <&ccu RST_BUS_TCON_TV0>;
+			reset-names = "lcd";
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				tcon_tv_in: port@0 {
+					reg = <0>;
+
+					tcon_tv_in_tcon_top_mixer0: endpoint {
+						remote-endpoint = <&tcon_top_mixer0_out_tcon_tv>;
+					};
+				};
+
+				tcon_tv_out: port@1 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <1>;
+
+					tcon_tv_out_tcon_top: endpoint@1 {
+						reg = <1>;
+						remote-endpoint = <&tcon_top_hdmi_in_tcon_tv>;
+					};
+				};
+			};
+		};
+
 		r_ccu: clock@7010000 {
 			compatible = "allwinner,sun50i-h6-r-ccu";
 			reg = <0x07010000 0x400>;
diff --git a/include/dt-bindings/clock/sun8i-tcon-top.h b/include/dt-bindings/clock/sun8i-tcon-top.h
new file mode 100644
index 0000000000..25164d7678
--- /dev/null
+++ b/include/dt-bindings/clock/sun8i-tcon-top.h
@@ -0,0 +1,11 @@
+/* SPDX-License-Identifier: (GPL-2.0+ OR MIT) */
+/* Copyright (C) 2018 Jernej Skrabec <jernej.skrabec@siol.net> */
+
+#ifndef _DT_BINDINGS_CLOCK_SUN8I_TCON_TOP_H_
+#define _DT_BINDINGS_CLOCK_SUN8I_TCON_TOP_H_
+
+#define CLK_TCON_TOP_TV0	0
+#define CLK_TCON_TOP_TV1	1
+#define CLK_TCON_TOP_DSI	2
+
+#endif /* _DT_BINDINGS_CLOCK_SUN8I_TCON_TOP_H_ */
