From d996492e1f700a9f0a104c50b126a022dee77dd6 Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Mon, 25 Dec 2017 12:04:02 +0800
Subject: [PATCH 20/34] phy: allwinner: add phy driver for USB3 PHY on
 Allwinner H6 SoC

Allwinner H6 SoC contains a USB3 PHY (with USB2 DP/DM lines also
controlled).

Add a driver for it.

The register operations in this driver is mainly extracted from the BSP
USB3 driver.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
Reviewed-by: Chen-Yu Tsai <wens@csie.org>
---
 drivers/phy/allwinner/Kconfig           |  12 ++
 drivers/phy/allwinner/Makefile          |   1 +
 drivers/phy/allwinner/phy-sun50i-usb3.c | 194 ++++++++++++++++++++++++
 3 files changed, 207 insertions(+)
 create mode 100644 drivers/phy/allwinner/phy-sun50i-usb3.c

diff --git a/drivers/phy/allwinner/Kconfig b/drivers/phy/allwinner/Kconfig
index fb1204bcc4548..2c363db177f20 100644
--- a/drivers/phy/allwinner/Kconfig
+++ b/drivers/phy/allwinner/Kconfig
@@ -41,3 +41,15 @@ config PHY_SUN9I_USB
 	  sun9i SoCs.
 
 	  This driver controls each individual USB 2 host PHY.
+
+config PHY_SUN50I_USB3
+	tristate "Allwinner sun50i SoC USB3 PHY driver"
+	depends on ARCH_SUNXI && HAS_IOMEM && OF
+	depends on RESET_CONTROLLER
+	select USB_COMMON
+	select GENERIC_PHY
+	help
+	  Enable this to support the USB3.0-capable transceiver that is
+	  part of some Allwinner sun50i SoCs.
+
+	  This driver controls each individual USB 2+3 host PHY combo.
diff --git a/drivers/phy/allwinner/Makefile b/drivers/phy/allwinner/Makefile
index 7d0053efbfaa6..59575a895779b 100644
--- a/drivers/phy/allwinner/Makefile
+++ b/drivers/phy/allwinner/Makefile
@@ -1,3 +1,4 @@
 obj-$(CONFIG_PHY_SUN4I_USB)		+= phy-sun4i-usb.o
 obj-$(CONFIG_PHY_SUN6I_MIPI_DPHY)	+= phy-sun6i-mipi-dphy.o
 obj-$(CONFIG_PHY_SUN9I_USB)		+= phy-sun9i-usb.o
+obj-$(CONFIG_PHY_SUN50I_USB3)		+= phy-sun50i-usb3.o
diff --git a/drivers/phy/allwinner/phy-sun50i-usb3.c b/drivers/phy/allwinner/phy-sun50i-usb3.c
new file mode 100644
index 0000000000000..226c99c2d664c
--- /dev/null
+++ b/drivers/phy/allwinner/phy-sun50i-usb3.c
@@ -0,0 +1,194 @@
+// SPDX-License-Identifier: GPL-2.0+
+/*
+ * Allwinner sun50i(H6) USB 3.0 phy driver
+ *
+ * Copyright (C) 2017 Icenowy Zheng <icenowy@aosc.io>
+ *
+ * Based on phy-sun9i-usb.c, which is:
+ *
+ * Copyright (C) 2014-2015 Chen-Yu Tsai <wens@csie.org>
+ *
+ * Based on code from Allwinner BSP, which is:
+ *
+ * Copyright (c) 2010-2015 Allwinner Technology Co., Ltd.
+ */
+
+#include <linux/clk.h>
+#include <linux/err.h>
+#include <linux/io.h>
+#include <linux/module.h>
+#include <linux/phy/phy.h>
+#include <linux/usb/of.h>
+#include <linux/platform_device.h>
+#include <linux/reset.h>
+
+/* Interface Status and Control Registers */
+#define SUNXI_ISCR			0x00
+#define SUNXI_PIPE_CLOCK_CONTROL	0x14
+#define SUNXI_PHY_TUNE_LOW		0x18
+#define SUNXI_PHY_TUNE_HIGH		0x1c
+#define SUNXI_PHY_EXTERNAL_CONTROL	0x20
+
+/* USB2.0 Interface Status and Control Register */
+#define SUNXI_ISCR_FORCE_VBUS		(3 << 12)
+
+/* PIPE Clock Control Register */
+#define SUNXI_PCC_PIPE_CLK_OPEN		(1 << 6)
+
+/* PHY External Control Register */
+#define SUNXI_PEC_EXTERN_VBUS		(3 << 1)
+#define SUNXI_PEC_SSC_EN		(1 << 24)
+#define SUNXI_PEC_REF_SSP_EN		(1 << 26)
+
+/* PHY Tune High Register */
+#define SUNXI_TX_DEEMPH_3P5DB(n)	((n) << 19)
+#define SUNXI_TX_DEEMPH_3P5DB_MASK	GENMASK(24, 19)
+#define SUNXI_TX_DEEMPH_6DB(n)		((n) << 13)
+#define SUNXI_TX_DEEMPH_6GB_MASK	GENMASK(18, 13)
+#define SUNXI_TX_SWING_FULL(n)		((n) << 6)
+#define SUNXI_TX_SWING_FULL_MASK	GENMASK(12, 6)
+#define SUNXI_LOS_BIAS(n)		((n) << 3)
+#define SUNXI_LOS_BIAS_MASK		GENMASK(5, 3)
+#define SUNXI_TXVBOOSTLVL(n)		((n) << 0)
+#define SUNXI_TXVBOOSTLVL_MASK		GENMASK(0, 2)
+
+struct sun50i_usb3_phy {
+	struct phy *phy;
+	void __iomem *regs;
+	struct reset_control *reset;
+	struct clk *clk;
+};
+
+static void sun50i_usb3_phy_open(struct sun50i_usb3_phy *phy)
+{
+	u32 val;
+
+	val = readl(phy->regs + SUNXI_PHY_EXTERNAL_CONTROL);
+	val |= SUNXI_PEC_EXTERN_VBUS;
+	val |= SUNXI_PEC_SSC_EN | SUNXI_PEC_REF_SSP_EN;
+	writel(val, phy->regs + SUNXI_PHY_EXTERNAL_CONTROL);
+
+	val = readl(phy->regs + SUNXI_PIPE_CLOCK_CONTROL);
+	val |= SUNXI_PCC_PIPE_CLK_OPEN;
+	writel(val, phy->regs + SUNXI_PIPE_CLOCK_CONTROL);
+
+	val = readl(phy->regs + SUNXI_ISCR);
+	val |= SUNXI_ISCR_FORCE_VBUS;
+	writel(val, phy->regs + SUNXI_ISCR);
+
+	/*
+	 * All the magic numbers written to the PHY_TUNE_{LOW_HIGH}
+	 * registers are directly taken from the BSP USB3 driver from
+	 * Allwiner.
+	 */
+	writel(0x0047fc87, phy->regs + SUNXI_PHY_TUNE_LOW);
+
+	val = readl(phy->regs + SUNXI_PHY_TUNE_HIGH);
+	val &= ~(SUNXI_TXVBOOSTLVL_MASK | SUNXI_LOS_BIAS_MASK |
+		 SUNXI_TX_SWING_FULL_MASK | SUNXI_TX_DEEMPH_6GB_MASK |
+		 SUNXI_TX_DEEMPH_3P5DB_MASK);
+	val |= SUNXI_TXVBOOSTLVL(0x7);
+	val |= SUNXI_LOS_BIAS(0x7);
+	val |= SUNXI_TX_SWING_FULL(0x55);
+	val |= SUNXI_TX_DEEMPH_6DB(0x20);
+	val |= SUNXI_TX_DEEMPH_3P5DB(0x15);
+	writel(val, phy->regs + SUNXI_PHY_TUNE_HIGH);
+}
+
+static int sun50i_usb3_phy_init(struct phy *_phy)
+{
+	struct sun50i_usb3_phy *phy = phy_get_drvdata(_phy);
+	int ret;
+
+	ret = clk_prepare_enable(phy->clk);
+	if (ret)
+		goto err_clk;
+
+	ret = reset_control_deassert(phy->reset);
+	if (ret)
+		goto err_reset;
+
+	sun50i_usb3_phy_open(phy);
+	return 0;
+
+err_reset:
+	clk_disable_unprepare(phy->clk);
+
+err_clk:
+	return ret;
+}
+
+static int sun50i_usb3_phy_exit(struct phy *_phy)
+{
+	struct sun50i_usb3_phy *phy = phy_get_drvdata(_phy);
+
+	reset_control_assert(phy->reset);
+	clk_disable_unprepare(phy->clk);
+
+	return 0;
+}
+
+static const struct phy_ops sun50i_usb3_phy_ops = {
+	.init		= sun50i_usb3_phy_init,
+	.exit		= sun50i_usb3_phy_exit,
+	.owner		= THIS_MODULE,
+};
+
+static int sun50i_usb3_phy_probe(struct platform_device *pdev)
+{
+	struct sun50i_usb3_phy *phy;
+	struct device *dev = &pdev->dev;
+	struct phy_provider *phy_provider;
+	struct resource *res;
+
+	phy = devm_kzalloc(dev, sizeof(*phy), GFP_KERNEL);
+	if (!phy)
+		return -ENOMEM;
+
+	phy->clk = devm_clk_get(dev, NULL);
+	if (IS_ERR(phy->clk)) {
+		dev_err(dev, "failed to get phy clock\n");
+		return PTR_ERR(phy->clk);
+	}
+
+	phy->reset = devm_reset_control_get(dev, NULL);
+	if (IS_ERR(phy->reset)) {
+		dev_err(dev, "failed to get reset control\n");
+		return PTR_ERR(phy->reset);
+	}
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	phy->regs = devm_ioremap_resource(dev, res);
+	if (IS_ERR(phy->regs))
+		return PTR_ERR(phy->regs);
+
+	phy->phy = devm_phy_create(dev, NULL, &sun50i_usb3_phy_ops);
+	if (IS_ERR(phy->phy)) {
+		dev_err(dev, "failed to create PHY\n");
+		return PTR_ERR(phy->phy);
+	}
+
+	phy_set_drvdata(phy->phy, phy);
+	phy_provider = devm_of_phy_provider_register(dev, of_phy_simple_xlate);
+
+	return PTR_ERR_OR_ZERO(phy_provider);
+}
+
+static const struct of_device_id sun50i_usb3_phy_of_match[] = {
+	{ .compatible = "allwinner,sun50i-h6-usb3-phy" },
+	{ },
+};
+MODULE_DEVICE_TABLE(of, sun50i_usb3_phy_of_match);
+
+static struct platform_driver sun50i_usb3_phy_driver = {
+	.probe	= sun50i_usb3_phy_probe,
+	.driver = {
+		.of_match_table	= sun50i_usb3_phy_of_match,
+		.name  = "sun50i-usb3-phy",
+	}
+};
+module_platform_driver(sun50i_usb3_phy_driver);
+
+MODULE_DESCRIPTION("Allwinner sun50i USB 3.0 phy driver");
+MODULE_AUTHOR("Icenowy Zheng <icenowy@aosc.io>");
+MODULE_LICENSE("GPL");
