From 9ea7a168e5cab7ad820439f1c595360e8c2415db Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Tue, 19 Feb 2019 21:54:24 +0100
Subject: [PATCH 01/34] rtc: sun6i: Add support for H6 RTC

It is mostly the same as on H5 and H3, but with slight differences
in features that are not yet supported by this driver, so we need
a different compatible, but we can re-use sun8i_h3_rtc_clk_init.

Some differences are already stated in the comments in existing code.
One other difference is that H6 has extra bit in LOSC_CTRL_REG, called
EXT_LOSC_EN to enable/disable external low speed crystal oscillator.

It also has bit EXT_LOSC_STA in LOSC_AUTO_SWT_STA_REG, to check whether
external low speed oscillator is working correctly.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 drivers/rtc/rtc-sun6i.c | 47 +++++++++++++++++++++++++++++++++++++++--
 1 file changed, 45 insertions(+), 2 deletions(-)

diff --git a/drivers/rtc/rtc-sun6i.c b/drivers/rtc/rtc-sun6i.c
index 11f56de521791..b0fbaa1837dd5 100644
--- a/drivers/rtc/rtc-sun6i.c
+++ b/drivers/rtc/rtc-sun6i.c
@@ -41,11 +41,15 @@
 /* Control register */
 #define SUN6I_LOSC_CTRL				0x0000
 #define SUN6I_LOSC_CTRL_KEY			(0x16aa << 16)
+#define SUN6I_LOSC_CTRL_AUTO_SWT_EN		BIT(14)
+#define SUN6I_LOSC_CTRL_AUTO_SWT_BYPASS		BIT(15)
 #define SUN6I_LOSC_CTRL_ALM_DHMS_ACC		BIT(9)
 #define SUN6I_LOSC_CTRL_RTC_HMS_ACC		BIT(8)
 #define SUN6I_LOSC_CTRL_RTC_YMD_ACC		BIT(7)
+#define SUN6I_LOSC_CTRL_EXT_LOSC_EN		BIT(4)
 #define SUN6I_LOSC_CTRL_EXT_OSC			BIT(0)
 #define SUN6I_LOSC_CTRL_ACC_MASK		GENMASK(9, 7)
+#define SUN6I_LOSC_CTRL_EXT_OSC_GSM             0x08
 
 #define SUN6I_LOSC_CLK_PRESCAL			0x0008
 
@@ -137,6 +141,8 @@ struct sun6i_rtc_clk_data {
 	unsigned int has_prescaler : 1;
 	unsigned int has_out_clk : 1;
 	unsigned int export_iosc : 1;
+	unsigned int has_losc_en : 1;
+	unsigned int has_auto_swt : 1;
 };
 
 struct sun6i_rtc_dev {
@@ -199,6 +205,10 @@ static int sun6i_rtc_osc_set_parent(struct clk_hw *hw, u8 index)
 	val &= ~SUN6I_LOSC_CTRL_EXT_OSC;
 	val |= SUN6I_LOSC_CTRL_KEY;
 	val |= index ? SUN6I_LOSC_CTRL_EXT_OSC : 0;
+	if (rtc->data->has_losc_en) {
+		val &= ~SUN6I_LOSC_CTRL_EXT_LOSC_EN;
+		val |= index ? SUN6I_LOSC_CTRL_EXT_LOSC_EN : 0;
+	}
 	writel(val, rtc->base + SUN6I_LOSC_CTRL);
 	spin_unlock_irqrestore(&rtc->lock, flags);
 
@@ -224,6 +234,7 @@ static void __init sun6i_rtc_clk_init(struct device_node *node,
 	const char *iosc_name = "rtc-int-osc";
 	const char *clkout_name = "osc32k-out";
 	const char *parents[2];
+	u32 reg;
 
 	rtc = kzalloc(sizeof(*rtc), GFP_KERNEL);
 	if (!rtc)
@@ -244,9 +255,23 @@ static void __init sun6i_rtc_clk_init(struct device_node *node,
 		goto err;
 	}
 
+	reg = SUN6I_LOSC_CTRL_KEY;
+	if (rtc->data->has_auto_swt) {
+		/* Bypass auto-switch to int osc, on ext losc failure */
+		reg |= SUN6I_LOSC_CTRL_AUTO_SWT_BYPASS;
+		writel(reg, rtc->base + SUN6I_LOSC_CTRL);
+	}
+
 	/* Switch to the external, more precise, oscillator */
-	writel(SUN6I_LOSC_CTRL_KEY | SUN6I_LOSC_CTRL_EXT_OSC,
-	       rtc->base + SUN6I_LOSC_CTRL);
+	reg |= SUN6I_LOSC_CTRL_EXT_OSC;
+	if (rtc->data->has_losc_en)
+		reg |= SUN6I_LOSC_CTRL_EXT_LOSC_EN;
+	writel(reg, rtc->base + SUN6I_LOSC_CTRL);
+
+	/* Set GSM with some delay, after switching to ext losc. */
+	udelay(10);
+	reg |= SUN6I_LOSC_CTRL_EXT_OSC_GSM;
+	writel(reg, rtc->base + SUN6I_LOSC_CTRL);
 
 	/* Yes, I know, this is ugly. */
 	sun6i_rtc = rtc;
@@ -354,6 +379,23 @@ CLK_OF_DECLARE_DRIVER(sun8i_h3_rtc_clk, "allwinner,sun8i-h3-rtc",
 CLK_OF_DECLARE_DRIVER(sun50i_h5_rtc_clk, "allwinner,sun50i-h5-rtc",
 		      sun8i_h3_rtc_clk_init);
 
+static const struct sun6i_rtc_clk_data sun50i_h6_rtc_data = {
+	.rc_osc_rate = 16000000,
+	.fixed_prescaler = 32,
+	.has_prescaler = 1,
+	.has_out_clk = 1,
+	.export_iosc = 1,
+	.has_losc_en = 1,
+	.has_auto_swt = 1,
+};
+
+static void __init sun50i_h6_rtc_clk_init(struct device_node *node)
+{
+	sun6i_rtc_clk_init(node, &sun50i_h6_rtc_data);
+}
+CLK_OF_DECLARE_DRIVER(sun50i_h6_rtc_clk, "allwinner,sun50i-h6-rtc",
+		      sun50i_h6_rtc_clk_init);
+
 static const struct sun6i_rtc_clk_data sun8i_v3_rtc_data = {
 	.rc_osc_rate = 32000,
 	.has_out_clk = 1,
@@ -683,6 +725,7 @@ static const struct of_device_id sun6i_rtc_dt_ids[] = {
 	{ .compatible = "allwinner,sun8i-h3-rtc" },
 	{ .compatible = "allwinner,sun8i-v3-rtc" },
 	{ .compatible = "allwinner,sun50i-h5-rtc" },
+	{ .compatible = "allwinner,sun50i-h6-rtc" },
 	{ /* sentinel */ },
 };
 MODULE_DEVICE_TABLE(of, sun6i_rtc_dt_ids);

From 80472652eff72ba5198dc5d678612fb91e411ed1 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Fri, 12 Apr 2019 13:32:05 +0200
Subject: [PATCH 02/34] arm64: dts: sun50i-h6: Add support for RTC and fix the
 clock tree

This patch adds RTC node and fixes the clock properties and nodes
to reflect the real clock tree.

The device nodes for the internal oscillator and osc32k are removed,
as these clocks are now provided by the RTC device. Clock references
are fixed accordingly, too.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi | 30 +++++++++++---------
 1 file changed, 16 insertions(+), 14 deletions(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
index c9e861a50a633..ae7977f3f054c 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
@@ -56,14 +56,6 @@
 		status = "disabled";
 	};
 
-	iosc: internal-osc-clk {
-		#clock-cells = <0>;
-		compatible = "fixed-clock";
-		clock-frequency = <16000000>;
-		clock-accuracy = <300000000>;
-		clock-output-names = "iosc";
-	};
-
 	osc24M: osc24M_clk {
 		#clock-cells = <0>;
 		compatible = "fixed-clock";
@@ -71,11 +63,11 @@
 		clock-output-names = "osc24M";
 	};
 
-	osc32k: osc32k_clk {
+	ext_osc32k: ext_osc32k_clk {
 		#clock-cells = <0>;
 		compatible = "fixed-clock";
 		clock-frequency = <32768>;
-		clock-output-names = "osc32k";
+		clock-output-names = "ext_osc32k";
 	};
 
 	psci {
@@ -186,7 +178,7 @@
 		ccu: clock@3001000 {
 			compatible = "allwinner,sun50i-h6-ccu";
 			reg = <0x03001000 0x1000>;
-			clocks = <&osc24M>, <&osc32k>, <&iosc>;
+			clocks = <&osc24M>, <&rtc 0>, <&rtc 2>;
 			clock-names = "hosc", "losc", "iosc";
 			#clock-cells = <1>;
 			#reset-cells = <1>;
@@ -199,7 +191,7 @@
 				     <GIC_SPI 53 IRQ_TYPE_LEVEL_HIGH>,
 				     <GIC_SPI 54 IRQ_TYPE_LEVEL_HIGH>,
 				     <GIC_SPI 59 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&ccu CLK_APB1>, <&osc24M>, <&osc32k>;
+			clocks = <&ccu CLK_APB1>, <&osc24M>, <&rtc 0>;
 			clock-names = "apb", "hosc", "losc";
 			gpio-controller;
 			#gpio-cells = <3>;
@@ -583,10 +575,20 @@
 			};
 		};
 
+		rtc: rtc@7000000 {
+			compatible = "allwinner,sun50i-h6-rtc";
+			reg = <0x07000000 0x400>;
+			interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>;
+			clock-output-names = "osc32k", "osc32k-out", "iosc";
+			clocks = <&ext_osc32k>;
+			#clock-cells = <1>;
+		};
+
 		r_ccu: clock@7010000 {
 			compatible = "allwinner,sun50i-h6-r-ccu";
 			reg = <0x07010000 0x400>;
-			clocks = <&osc24M>, <&osc32k>, <&iosc>,
+			clocks = <&osc24M>, <&rtc 0>, <&rtc 2>,
 				 <&ccu CLK_PLL_PERIPH0>;
 			clock-names = "hosc", "losc", "iosc", "pll-periph";
 			#clock-cells = <1>;
@@ -607,7 +609,7 @@
 			reg = <0x07022000 0x400>;
 			interrupts = <GIC_SPI 105 IRQ_TYPE_LEVEL_HIGH>,
 				     <GIC_SPI 111 IRQ_TYPE_LEVEL_HIGH>;
-			clocks = <&r_ccu CLK_R_APB1>, <&osc24M>, <&osc32k>;
+			clocks = <&r_ccu CLK_R_APB1>, <&osc24M>, <&rtc 0>;
 			clock-names = "apb", "hosc", "losc";
 			gpio-controller;
 			#gpio-cells = <3>;

From de4dc594bb3cb124d21fd7550ca0497c7fa22ff0 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Thu, 11 Apr 2019 11:20:54 +0200
Subject: [PATCH 07/34] arm64: dts: h6: Make mmc0_pins the default for &mmc0

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
index ae7977f3f054c..91623a8cd2a08 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
@@ -254,6 +254,8 @@
 			resets = <&ccu RST_BUS_MMC0>;
 			reset-names = "ahb";
 			interrupts = <GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&mmc0_pins>;
 			status = "disabled";
 			#address-cells = <1>;
 			#size-cells = <0>;

From 45bbbb485eb478df71079fd69f7ee8e48d0b0809 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Thu, 11 Apr 2019 11:11:21 +0200
Subject: [PATCH 08/34] arm64: dts: allwinner: h6: Add Orange Pi 3 DTS

Orange Pi 3 is a H6 based SBC made by Xulong, released in January 2019. It
has the following features:

- Allwinner H6 quad-core 64-bit ARM Cortex-A53
- GPU Mali-T720
- 1GB or 2GB LPDDR3 RAM
- AXP805 PMIC
- AP6256 Wifi/BT 5.0
- USB 2.0 host port (A)
- USB 2.0 micro usb, OTG
- USB 3.0 Host + 4 port USB hub (GL3510)
- Gigabit Ethernet (Realtek RTL8211E phy)
- HDMI 2.0 port
- soldered eMMC (optional)
- 3x LED (one is on the bottom)
- microphone
- audio jack
- PCIe

Add basic support for the board.

Signed-off-by: Ondrej Jirman <megous@megous.com>
Signed-off-by: Maxime Ripard <maxime.ripard@bootlin.com>
---
 arch/arm64/boot/dts/allwinner/Makefile        |   1 +
 .../dts/allwinner/sun50i-h6-orangepi-3.dts    | 215 ++++++++++++++++++
 2 files changed, 216 insertions(+)
 create mode 100644 arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts

diff --git a/arch/arm64/boot/dts/allwinner/Makefile b/arch/arm64/boot/dts/allwinner/Makefile
index 0b09171110994..13a7e87bc35cc 100644
--- a/arch/arm64/boot/dts/allwinner/Makefile
+++ b/arch/arm64/boot/dts/allwinner/Makefile
@@ -19,6 +19,7 @@ dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-orangepi-pc2.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-orangepi-prime.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-orangepi-zero-plus.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-orangepi-zero-plus2.dtb
+dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h6-orangepi-3.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h6-orangepi-lite2.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h6-orangepi-one-plus.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h6-pine-h64.dtb
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
new file mode 100644
index 0000000000000..17d4969901086
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
@@ -0,0 +1,229 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+/*
+ * Copyright (C) 2019 Ondřej Jirman <megous@megous.com>
+ */
+
+/dts-v1/;
+
+#include "sun50i-h6.dtsi"
+
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	model = "OrangePi 3";
+	compatible = "xunlong,orangepi-3", "allwinner,sun50i-h6";
+
+	aliases {
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		power {
+			label = "orangepi:red:power";
+			gpios = <&r_pio 0 4 GPIO_ACTIVE_HIGH>; /* PL4 */
+			default-state = "on";
+		};
+
+		status {
+			label = "orangepi:green:status";
+			gpios = <&r_pio 0 7 GPIO_ACTIVE_HIGH>; /* PL7 */
+		};
+	};
+
+	reg_vcc5v: vcc5v {
+		/* board wide 5V supply directly from the DC jack */
+		compatible = "regulator-fixed";
+		regulator-name = "vcc-5v";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-always-on;
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&reg_dcdca>;
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&ehci3 {
+	status = "okay";
+};
+
+&gpu {
+	mali-supply = <&reg_dcdcc>;
+};
+
+&mmc0 {
+	vmmc-supply = <&reg_cldo1>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>; /* PF6 */
+	bus-width = <4>;
+	status = "okay";
+};
+
+&mmc2 {
+      pinctrl-names = "default";
+      pinctrl-0 = <&mmc2_pins>;
+      vmmc-supply = <&reg_cldo1>;
+      non-removable;
+      cap-mmc-hw-reset;
+      bus-width = <8>;
+      status = "okay";
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&ohci3 {
+	status = "okay";
+};
+
+&pio {
+	vcc-pc-supply = <&reg_bldo2>;
+	vcc-pd-supply = <&reg_cldo1>;
+};
+
+&r_i2c {
+	status = "okay";
+
+	axp805: pmic@36 {
+		compatible = "x-powers,axp805", "x-powers,axp806";
+		reg = <0x36>;
+		interrupt-parent = <&r_intc>;
+		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
+		interrupt-controller;
+		#interrupt-cells = <1>;
+		x-powers,self-working-mode;
+		vina-supply = <&reg_vcc5v>;
+		vinb-supply = <&reg_vcc5v>;
+		vinc-supply = <&reg_vcc5v>;
+		vind-supply = <&reg_vcc5v>;
+		vine-supply = <&reg_vcc5v>;
+		aldoin-supply = <&reg_vcc5v>;
+		bldoin-supply = <&reg_vcc5v>;
+		cldoin-supply = <&reg_vcc5v>;
+
+		regulators {
+			reg_aldo1: aldo1 {
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-pl-led-ir";
+			};
+
+			reg_aldo2: aldo2 {
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc33-audio-tv-ephy-mac";
+			};
+
+			/* ALDO3 is shorted to CLDO1 */
+			reg_aldo3: aldo3 {
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc33-io-pd-emmc-sd-usb-uart-1";
+			};
+
+			reg_bldo1: bldo1 {
+				regulator-always-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcc18-dram-bias-pll";
+			};
+
+			reg_bldo2: bldo2 {
+				regulator-always-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcc-efuse-pcie-hdmi-pc";
+			};
+
+			bldo3 {
+				/* unused */
+			};
+
+			bldo4 {
+				/* unused */
+			};
+
+			reg_cldo1: cldo1 {
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc33-io-pd-emmc-sd-usb-uart-2";
+			};
+
+			cldo2 {
+				/* unused */
+			};
+
+			cldo3 {
+				/* unused */
+			};
+
+			reg_dcdca: dcdca {
+				regulator-always-on;
+				regulator-min-microvolt = <800000>;
+				regulator-max-microvolt = <1160000>;
+				regulator-name = "vdd-cpu";
+			};
+
+			reg_dcdcc: dcdcc {
+				regulator-min-microvolt = <810000>;
+				regulator-max-microvolt = <1080000>;
+				regulator-name = "vdd-gpu";
+			};
+
+			reg_dcdcd: dcdcd {
+				regulator-always-on;
+				regulator-min-microvolt = <960000>;
+				regulator-max-microvolt = <960000>;
+				regulator-name = "vdd-sys";
+			};
+
+			reg_dcdce: dcdce {
+				regulator-always-on;
+				regulator-min-microvolt = <1200000>;
+				regulator-max-microvolt = <1200000>;
+				regulator-name = "vcc-dram";
+			};
+
+			sw {
+				/* unused */
+			};
+		};
+	};
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_ph_pins>;
+	status = "okay";
+};
+
+&usb2otg {
+	/*
+	 * This board doesn't have a controllable VBUS even though it
+	 * does have an ID pin. Using it as anything but a USB host is
+	 * unsafe.
+	 */
+	dr_mode = "host";
+	status = "okay";
+};
+
+&usb2phy {
+	usb0_id_det-gpios = <&pio 2 15 GPIO_ACTIVE_HIGH>; /* PC15 */
+	usb0_vbus-supply = <&reg_vcc5v>;
+	usb3_vbus-supply = <&reg_vcc5v>;
+	status = "okay";
+};

From 2a87073bd0857fd9707de2ac96cb04d6d9e0e288 Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Tue, 9 Jan 2018 23:58:12 +0800
Subject: [PATCH 10/34] net: stmmac: sun8i: force select external PHY when no
 internal one

From e6d3f7e02d211522c7f1cc09df946292601b55b6 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Wed, 27 Mar 2019 13:21:06 +0100
Subject: [PATCH 13/34] arm64: dts: allwinner: orange-pi-3: Enable ethernet

Orange Pi 3 has two regulators that power the Realtek RTL8211E. According
to the phy datasheet, both regulators need to be enabled at the same time,
but we can only specify a single phy-supply in the DT.

This can be achieved by making one regulator depedning on the other via
vin-supply. While it's not a technically correct description of the
hardware, it achieves the purpose.

All values of RX/TX delay were tested exhaustively and a middle one of the
working values was chosen.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 .../dts/allwinner/sun50i-h6-orangepi-3.dts    | 44 +++++++++++++++++++
 1 file changed, 44 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
index 17d4969901086..6d6b1f66796d9 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
@@ -15,6 +15,7 @@
 
 	aliases {
 		serial0 = &uart0;
+		ethernet0 = &emac;
 	};
 
 	chosen {
@@ -44,6 +45,27 @@
 		regulator-max-microvolt = <5000000>;
 		regulator-always-on;
 	};
+
+	/*
+	 * The board uses 2.5V RGMII signalling. Power sequence to enable
+	 * the phy is to enable GMAC-2V5 and GMAC-3V3 (aldo2) power rails
+	 * at the same time and to wait 100ms.
+	 */
+	reg_gmac_2v5: gmac-2v5 {
+		compatible = "regulator-fixed";
+		regulator-name = "gmac-2v5";
+		regulator-min-microvolt = <2500000>;
+		regulator-max-microvolt = <2500000>;
+		startup-delay-us = <100000>;
+		enable-active-high;
+		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>; /* PD6 */
+
+		/* The real parent of gmac-2v5 is reg_vcc5v, but we need to
+		 * enable two regulators to power the phy. This is one way
+		 * to achieve that.
+		 */
+		vin-supply = <&reg_aldo2>; /* GMAC-3V3 */
+	};
 };
 
 &cpu0 {
@@ -58,6 +80,28 @@
 	status = "okay";
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&ext_rgmii_pins>;
+	phy-mode = "rgmii";
+	phy-handle = <&ext_rgmii_phy>;
+	phy-supply = <&reg_gmac_2v5>;
+	allwinner,rx-delay-ps = <1500>;
+	allwinner,tx-delay-ps = <700>;
+	status = "okay";
+};
+
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+
+		reset-gpios = <&pio 3 14 GPIO_ACTIVE_LOW>; /* PD14 */
+		reset-assert-us = <15000>;
+		reset-deassert-us = <40000>;
+	};
+};
+
 &mmc0 {
 	vmmc-supply = <&reg_cldo1>;
 	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>; /* PF6 */

From b641bc59468e93ab57fd016ad36b037f3890b994 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Tue, 26 Mar 2019 15:06:37 +0100
Subject: [PATCH 15/34] drm: sun4i: Add support for enabling DDC I2C bus power
 to dw_hdmi glue

Orange Pi 3 board requires enabling DDC I2C bus via some GPIO connected
transistors, before the bus can be used.

Model this as a power supply for DDC bus on the HDMI connector connected
to the output port (port 1) of the HDMI controller.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 drivers/gpu/drm/sun4i/sun8i_dw_hdmi.c | 60 ++++++++++++++++++++++++++-
 drivers/gpu/drm/sun4i/sun8i_dw_hdmi.h |  2 +
 2 files changed, 60 insertions(+), 2 deletions(-)

diff --git a/drivers/gpu/drm/sun4i/sun8i_dw_hdmi.c b/drivers/gpu/drm/sun4i/sun8i_dw_hdmi.c
index 39d8509d96a0d..1b6ffba41177f 100644
--- a/drivers/gpu/drm/sun4i/sun8i_dw_hdmi.c
+++ b/drivers/gpu/drm/sun4i/sun8i_dw_hdmi.c
@@ -98,6 +98,30 @@ static u32 sun8i_dw_hdmi_find_possible_crtcs(struct drm_device *drm,
 	return crtcs;
 }
 
+static int sun8i_dw_hdmi_find_connector_pdev(struct device *dev,
+					     struct platform_device **pdev_out)
+{
+	struct platform_device* pdev;
+	struct device_node *remote;
+
+	remote = of_graph_get_remote_node(dev->of_node, 1, -1);
+	if (!remote)
+		return -ENODEV;
+
+	if (!of_device_is_compatible(remote, "hdmi-connector")) {
+		of_node_put(remote);
+		return -ENODEV;
+	}
+
+	pdev = of_find_device_by_node(remote);
+	of_node_put(remote);
+	if (!pdev)
+		return -ENODEV;
+
+	*pdev_out = pdev;
+	return 0;
+}
+
 static int sun8i_dw_hdmi_bind(struct device *dev, struct device *master,
 			      void *data)
 {
@@ -151,16 +175,34 @@ static int sun8i_dw_hdmi_bind(struct device *dev, struct device *master,
 		return PTR_ERR(hdmi->regulator);
 	}
 
+	ret = sun8i_dw_hdmi_find_connector_pdev(dev, &hdmi->connector_pdev);
+	if (!ret) {
+		hdmi->ddc_regulator = regulator_get(&hdmi->connector_pdev->dev, "ddc");
+		if (IS_ERR(hdmi->ddc_regulator)) {
+			platform_device_put(hdmi->connector_pdev);
+			dev_err(dev, "Couldn't get ddc regulator\n");
+			return PTR_ERR(hdmi->ddc_regulator);
+		}
+	}
+
 	ret = regulator_enable(hdmi->regulator);
 	if (ret) {
 		dev_err(dev, "Failed to enable regulator\n");
-		return ret;
+		goto err_unref_ddc_regulator;
+	}
+
+	if (hdmi->ddc_regulator) {
+		ret = regulator_enable(hdmi->ddc_regulator);
+		if (ret) {
+			dev_err(dev, "Failed to enable ddc regulator\n");
+			goto err_disable_regulator;
+		}
 	}
 
 	ret = reset_control_deassert(hdmi->rst_ctrl);
 	if (ret) {
 		dev_err(dev, "Could not deassert ctrl reset control\n");
-		goto err_disable_regulator;
+		goto err_disable_ddc_regulator;
 	}
 
 	ret = clk_prepare_enable(hdmi->clk_tmds);
@@ -213,8 +255,15 @@ static int sun8i_dw_hdmi_bind(struct device *dev, struct device *master,
 	clk_disable_unprepare(hdmi->clk_tmds);
 err_assert_ctrl_reset:
 	reset_control_assert(hdmi->rst_ctrl);
+err_disable_ddc_regulator:
+	if (hdmi->ddc_regulator)
+		regulator_disable(hdmi->ddc_regulator);
 err_disable_regulator:
 	regulator_disable(hdmi->regulator);
+err_unref_ddc_regulator:
+	if (hdmi->ddc_regulator)
+		regulator_put(hdmi->ddc_regulator);
+	platform_device_put(hdmi->connector_pdev);
 
 	return ret;
 }
@@ -229,6 +278,13 @@ static void sun8i_dw_hdmi_unbind(struct device *dev, struct device *master,
 	clk_disable_unprepare(hdmi->clk_tmds);
 	reset_control_assert(hdmi->rst_ctrl);
 	regulator_disable(hdmi->regulator);
+
+	if (hdmi->ddc_regulator) {
+		regulator_disable(hdmi->ddc_regulator);
+		regulator_put(hdmi->ddc_regulator);
+	}
+
+	platform_device_put(hdmi->connector_pdev);
 }
 
 static const struct component_ops sun8i_dw_hdmi_ops = {
diff --git a/drivers/gpu/drm/sun4i/sun8i_dw_hdmi.h b/drivers/gpu/drm/sun4i/sun8i_dw_hdmi.h
index 720c5aa8adc14..60f5200aee73b 100644
--- a/drivers/gpu/drm/sun4i/sun8i_dw_hdmi.h
+++ b/drivers/gpu/drm/sun4i/sun8i_dw_hdmi.h
@@ -188,8 +188,10 @@ struct sun8i_dw_hdmi {
 	struct sun8i_hdmi_phy		*phy;
 	struct dw_hdmi_plat_data	plat_data;
 	struct regulator		*regulator;
+	struct regulator		*ddc_regulator;
 	const struct sun8i_dw_hdmi_quirks *quirks;
 	struct reset_control		*rst_ctrl;
+	struct platform_device		*connector_pdev;
 };
 
 static inline struct sun8i_dw_hdmi *

From c1d7c7796ea7e76829c71b993c7531f23c0f5913 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Tue, 9 Apr 2019 01:41:58 +0200
Subject: [PATCH 16/34] arm64: dts: allwinner: orange-pi-3: Enable HDMI output

Orange Pi 3 has a DDC_CEC_EN signal connected to PH2, that enables the DDC
I2C bus voltage shifter. Before EDID can be read, we need to pull PH2 high.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 .../dts/allwinner/sun50i-h6-orangepi-3.dts    | 35 +++++++++++++++++++
 1 file changed, 35 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
index 6d6b1f66796d9..58a6635c909e3 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
@@ -22,6 +22,18 @@
 		stdout-path = "serial0:115200n8";
 	};
 
+	connector {
+		compatible = "hdmi-connector";
+		type = "a";
+		ddc-supply = <&reg_ddc>;
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
 	leds {
 		compatible = "gpio-leds";
 
@@ -37,6 +49,15 @@
 		};
 	};
 
+	reg_ddc: ddc-io {
+		compatible = "regulator-fixed";
+		regulator-name = "ddc-io";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		enable-active-high;
+		gpio = <&pio 7 2 GPIO_ACTIVE_HIGH>; /* PH2 */
+	};
+
 	reg_vcc5v: vcc5v {
 		/* board wide 5V supply directly from the DC jack */
 		compatible = "regulator-fixed";
@@ -72,6 +93,10 @@
 	cpu-supply = <&reg_dcdca>;
 };
 
+&de {
+	status = "okay";
+};
+
 &ehci0 {
 	status = "okay";
 };
@@ -91,6 +116,16 @@
 	status = "okay";
 };
 
+&hdmi {
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
 &mdio {
 	ext_rgmii_phy: ethernet-phy@1 {
 		compatible = "ethernet-phy-ieee802.3-c22";

From 756b0ba6d79844dbc04c6c4ea0fc25b52209721a Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Fri, 5 Apr 2019 22:21:00 +0200
Subject: [PATCH 17/34] brcmfmac: Loading the correct firmware for brcm43456

SDIO based brcm43456 is currently misdetected as brcm43455 and the wrong
firmware name is used. Correct the detection and load the correct firmware
file. Chiprev for brcm43456 is "9".

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c | 4 +++-
 1 file changed, 3 insertions(+), 1 deletion(-)

diff --git a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
index 4d104ab80fd8e..50e56fd056baa 100644
--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
@@ -622,6 +622,7 @@ BRCMF_FW_DEF(43430A0, "brcmfmac43430a0-sdio");
 /* Note the names are not postfixed with a1 for backward compatibility */
 BRCMF_FW_DEF(43430A1, "brcmfmac43430-sdio");
 BRCMF_FW_DEF(43455, "brcmfmac43455-sdio");
+BRCMF_FW_DEF(43456, "brcmfmac43456-sdio");
 BRCMF_FW_DEF(4354, "brcmfmac4354-sdio");
 BRCMF_FW_DEF(4356, "brcmfmac4356-sdio");
 BRCMF_FW_DEF(4373, "brcmfmac4373-sdio");
@@ -642,7 +643,8 @@ static const struct brcmf_firmware_mapping brcmf_sdio_fwnames[] = {
 	BRCMF_FW_ENTRY(BRCM_CC_4339_CHIP_ID, 0xFFFFFFFF, 4339),
 	BRCMF_FW_ENTRY(BRCM_CC_43430_CHIP_ID, 0x00000001, 43430A0),
 	BRCMF_FW_ENTRY(BRCM_CC_43430_CHIP_ID, 0xFFFFFFFE, 43430A1),
-	BRCMF_FW_ENTRY(BRCM_CC_4345_CHIP_ID, 0xFFFFFFC0, 43455),
+	BRCMF_FW_ENTRY(BRCM_CC_4345_CHIP_ID, 0x00000200, 43456),
+	BRCMF_FW_ENTRY(BRCM_CC_4345_CHIP_ID, 0xFFFFFDC0, 43455),
 	BRCMF_FW_ENTRY(BRCM_CC_4354_CHIP_ID, 0xFFFFFFFF, 4354),
 	BRCMF_FW_ENTRY(BRCM_CC_4356_CHIP_ID, 0xFFFFFFFF, 4356),
 	BRCMF_FW_ENTRY(CY_CC_4373_CHIP_ID, 0xFFFFFFFF, 4373),

From 5bf634f86c57f59f5c4a4fade9ccfe582334464f Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Mon, 18 Feb 2019 13:53:18 +0100
Subject: [PATCH 18/34] arm64: dts: allwinner: h6: Add MMC1 pins

MMC1 is used on some H6 boards we want to support. Typical use is 4-bit
SDIO interface with a WiFi chip. Add pin definitions for this use case.

As this is the only possible configration for mmc1, make it the default
one, too.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi | 11 +++++++++++
 1 file changed, 11 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
index 91623a8cd2a08..c5c0608e67403 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
@@ -219,6 +219,15 @@
 				bias-pull-up;
 			};
 
+			/omit-if-no-ref/
+			mmc1_pins: mmc1-pins {
+				pins = "PG0", "PG1", "PG2", "PG3",
+				       "PG4", "PG5";
+				function = "mmc1";
+				drive-strength = <30>;
+				bias-pull-up;
+			};
+
 			mmc2_pins: mmc2-pins {
 				pins = "PC1", "PC4", "PC5", "PC6",
 				       "PC7", "PC8", "PC9", "PC10",
@@ -270,6 +279,8 @@
 			resets = <&ccu RST_BUS_MMC1>;
 			reset-names = "ahb";
 			interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&mmc1_pins>;
 			status = "disabled";
 			#address-cells = <1>;
 			#size-cells = <0>;

From 200cf18794214700f023440021cb7fd40dcc0f01 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Tue, 9 Apr 2019 00:16:35 +0200
Subject: [PATCH 19/34] arm64: dts: allwinner: orange-pi-3: Enable WiFi

Orange Pi 3 has AP6256 WiFi/BT module. WiFi part of the module is called
bcm43356 and can be used with the brcmfmac driver. The module is powered by
the two always on regulators (not AXP805).

WiFi uses a PG port with 1.8V voltage level signals. SoC needs to be
configured so that it sets up an 1.8V input bias on this port. This is done
by the pio driver by reading the vcc-pg-supply voltage.

You'll need a fw_bcm43456c5_ag.bin firmware file and nvram.txt
configuration that can be found in the Xulongs's repository for H6:

https://github.com/orangepi-xunlong/OrangePiH6_external/tree/master/ap6256

Mainline brcmfmac driver expects the firmware and nvram at the following
paths relative to the firmware directory:

  brcm/brcmfmac43456-sdio.bin
  brcm/brcmfmac43456-sdio.txt

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 .../dts/allwinner/sun50i-h6-orangepi-3.dts    | 48 +++++++++++++++++++
 1 file changed, 48 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
index 58a6635c909e3..f795362f5b77e 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
@@ -67,6 +67,26 @@
 		regulator-always-on;
 	};
 
+	reg_vcc33_wifi: vcc33-wifi {
+		/* Always on 3.3V regulator for WiFi and BT */
+		compatible = "regulator-fixed";
+		regulator-name = "vcc33-wifi";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-always-on;
+		vin-supply = <&reg_vcc5v>;
+	};
+
+	reg_vcc_wifi_io: vcc-wifi-io {
+		/* Always on 1.8V/300mA regulator for WiFi and BT IO */
+		compatible = "regulator-fixed";
+		regulator-name = "vcc-wifi-io";
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+		regulator-always-on;
+		vin-supply = <&reg_vcc33_wifi>;
+	};
+
 	/*
 	 * The board uses 2.5V RGMII signalling. Power sequence to enable
 	 * the phy is to enable GMAC-2V5 and GMAC-3V3 (aldo2) power rails
@@ -87,6 +107,14 @@
 		 */
 		vin-supply = <&reg_aldo2>; /* GMAC-3V3 */
 	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		clocks = <&rtc 1>;
+		clock-names = "ext_clock";
+		reset-gpios = <&r_pio 1 3 GPIO_ACTIVE_LOW>; /* PM3 */
+		post-power-on-delay-ms = <200>;
+	};
 };
 
 &cpu0 {
@@ -144,6 +172,25 @@
 	status = "okay";
 };
 
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins>;
+	vmmc-supply = <&reg_vcc33_wifi>;
+	vqmmc-supply = <&reg_vcc_wifi_io>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	brcm: sdio-wifi@1 {
+		reg = <1>;
+		compatible = "brcm,bcm4329-fmac";
+		interrupt-parent = <&r_pio>;
+		interrupts = <1 0 IRQ_TYPE_LEVEL_LOW>; /* PM0 */
+		interrupt-names = "host-wake";
+	};
+};
+
 &ohci0 {
 	status = "okay";
 };
@@ -155,6 +202,7 @@
 &pio {
 	vcc-pc-supply = <&reg_bldo2>;
 	vcc-pd-supply = <&reg_cldo1>;
+	vcc-pg-supply = <&reg_vcc_wifi_io>;
 };
 
 &r_i2c {

From 5fd2d3bd956cc875d07433454f18dcbc14e120d5 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Tue, 26 Mar 2019 15:14:14 +0100
Subject: [PATCH 24/34] bluetooth: bcm: Add support for loading firmware for
 BCM4345C5

WIP

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 drivers/bluetooth/btbcm.c   | 3 +++
 drivers/bluetooth/hci_bcm.c | 1 +
 2 files changed, 4 insertions(+)

diff --git a/drivers/bluetooth/btbcm.c b/drivers/bluetooth/btbcm.c
index d5d6e6e5da3bf..a58bf860bcbfc 100644
--- a/drivers/bluetooth/btbcm.c
+++ b/drivers/bluetooth/btbcm.c
@@ -37,6 +37,7 @@
 #define BDADDR_BCM4324B3 (&(bdaddr_t) {{0x00, 0x00, 0x00, 0xb3, 0x24, 0x43}})
 #define BDADDR_BCM4330B1 (&(bdaddr_t) {{0x00, 0x00, 0x00, 0xb1, 0x30, 0x43}})
 #define BDADDR_BCM43341B (&(bdaddr_t) {{0xac, 0x1f, 0x00, 0x1b, 0x34, 0x43}})
+#define BDADDR_BCM4345C5 (&(bdaddr_t) {{0xac, 0x1f, 0x00, 0xc5, 0x45, 0x43}})
 
 int btbcm_check_bdaddr(struct hci_dev *hdev)
 {
@@ -82,6 +83,7 @@ int btbcm_check_bdaddr(struct hci_dev *hdev)
 	    !bacmp(&bda->bdaddr, BDADDR_BCM4324B3) ||
 	    !bacmp(&bda->bdaddr, BDADDR_BCM4330B1) ||
+	    !bacmp(&bda->bdaddr, BDADDR_BCM4345C5) ||
 	    !bacmp(&bda->bdaddr, BDADDR_BCM43430A0) ||
 	    !bacmp(&bda->bdaddr, BDADDR_BCM43341B)) {
 		bt_dev_info(hdev, "BCM: Using default device address (%pMR)",
 			    &bda->bdaddr);
@@ -339,6 +341,7 @@ static const struct bcm_subver_table bcm_uart_subver_table[] = {
 	{ 0x2122, "BCM4343A0"	},	/* 001.001.034 */
 	{ 0x2209, "BCM43430A1"  },	/* 001.002.009 */
 	{ 0x6119, "BCM4345C0"	},	/* 003.001.025 */
+	{ 0x6606, "BCM4345C5"	},	/* 003.006.006 */
 	{ 0x230f, "BCM4356A2"	},	/* 001.003.015 */
 	{ 0x220e, "BCM20702A1"  },	/* 001.002.014 */
 	{ 0x4217, "BCM4329B1"   },	/* 002.002.023 */
diff --git a/drivers/bluetooth/hci_bcm.c b/drivers/bluetooth/hci_bcm.c
index ddbe518c3e5b8..d5d5ddc3cf1b8 100644
--- a/drivers/bluetooth/hci_bcm.c
+++ b/drivers/bluetooth/hci_bcm.c
@@ -1419,6 +1419,7 @@ static void bcm_serdev_remove(struct serdev_device *serdev)
 #ifdef CONFIG_OF
 static const struct of_device_id bcm_bluetooth_of_match[] = {
 	{ .compatible = "brcm,bcm20702a1" },
+	{ .compatible = "brcm,bcm4345c5" },
 	{ .compatible = "brcm,bcm4330-bt" },
 	{ .compatible = "brcm,bcm43438-bt" },
 	{ },

From d5626d424fbdc9dde5f8a2e525e88de33fc898cc Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Fri, 12 Apr 2019 13:24:26 +0200
Subject: [PATCH 25/34] bluetooth: hci_bcm: Give more time to come out of reset

Some devices need more time to come out of reset (eg. BCM4345).
Increase the post-reset delay. I don't have datasheet, so rather
be safe than to get intermittent failures during probe.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 drivers/bluetooth/hci_bcm.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/bluetooth/hci_bcm.c b/drivers/bluetooth/hci_bcm.c
index d5d5ddc3cf1b8..9eacaf8f72ec3 100644
--- a/drivers/bluetooth/hci_bcm.c
+++ b/drivers/bluetooth/hci_bcm.c
@@ -263,7 +263,7 @@ static int bcm_gpio_set_power(struct bcm_device *dev, bool powered)
 	}
 
 	/* wait for device to power on and come out of reset */
-	usleep_range(10000, 20000);
+	usleep_range(50000, 60000);
 
 	dev->res_enabled = powered;
 

From 5141fbafc9bf5f1a7cbb6923bc719f595ce54dae Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Mon, 25 Dec 2017 12:10:06 +0800
Subject: [PATCH 26/34] arm64: dts: allwinner: h6: add USB3 device nodes

Allwinner H6 SoC features USB3 functionality, with a DWC3 controller and
a custom PHY.

Add device tree nodes for them.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
Reviewed-by: Chen-Yu Tsai <wens@csie.org>
---
 arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi | 32 ++++++++++++++++++++
 1 file changed, 32 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
index c5c0608e67403..38784589558ca 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
@@ -420,6 +420,38 @@
 			status = "disabled";
 		};
 
+		dwc3: dwc3@5200000 {
+			compatible = "snps,dwc3";
+			reg = <0x05200000 0x10000>;
+			interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_XHCI>,
+				 <&ccu CLK_BUS_XHCI>,
+				 <&rtc 0>;
+			clock-names = "ref", "bus_early", "suspend";
+			resets = <&ccu RST_BUS_XHCI>;
+			/*
+			 * The datasheet of the chip doesn't declare the
+			 * peripheral function, and there's no boards known
+			 * to have a USB Type-B port routed to the port.
+			 * In addition, no one has tested the peripheral
+			 * function yet.
+			 * So set the dr_mode to "host" in the DTSI file.
+			 */
+			dr_mode = "host";
+			phys = <&usb3phy>;
+			phy-names = "usb3-phy";
+			status = "disabled";
+		};
+
+		usb3phy: phy@5210000 {
+			compatible = "allwinner,sun50i-h6-usb3-phy";
+			reg = <0x5210000 0x10000>;
+			clocks = <&ccu CLK_USB_PHY1>;
+			resets = <&ccu RST_USB_PHY1>;
+			#phy-cells = <0>;
+			status = "disabled";
+		};
+
 		ehci3: usb@5311000 {
 			compatible = "allwinner,sun50i-h6-ehci", "generic-ehci";
 			reg = <0x05311000 0x100>;

FFrom 19ed1005f6d1d2955c9e3e88c3fe037b46284ca8 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Tue, 26 Mar 2019 15:13:34 +0100
Subject: [PATCH 32/34] arm64: dts: allwinner: h6: Add pin configs for uart1

Orange Pi 3 uses UART1 for bluetooth. Add pinconfigs so that
we can use them.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi | 10 ++++++++++
 1 file changed, 10 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
index 5c5b1240c7790..dc785da9ce0a2 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
@@ -322,6 +322,16 @@
 				pins = "PH0", "PH1";
 				function = "uart0";
 			};
+
+			uart1_pins: uart1-pins {
+				pins = "PG6", "PG7";
+				function = "uart1";
+			};
+
+			uart1_rts_cts_pins: uart1-rts-cts-pins {
+				pins = "PG8", "PG9";
+				function = "uart1";
+			};
 		};
 
 		gic: interrupt-controller@3021000 {

From 785248f1b1d89bbd8a25435f873bfa91c27fa123 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Wed, 27 Mar 2019 13:48:59 +0100
Subject: [PATCH 33/34] arm64: dts: allwinner: orange-pi-3: Enable UART1 /
 Bluetooth

The board contains AP6256 WiFi/BT module that has its bluetooth
part connected to SoC's UART1 port. Enable this port, and add
node for the bluetooth device.

Bluetooth part is named bcm4345c5.

You'll need a BCM4345C5.hcd firmware file that can be found in
the Xulongs's repository for H6:

https://github.com/orangepi-xunlong/OrangePiH6_external/tree/master/ap6256

Mainline brcmbt driver expects the firmware at the following path
relative to the firmware directory:

  brcm/BCM4345C5.hcd

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 .../dts/allwinner/sun50i-h6-orangepi-3.dts    | 19 +++++++++++++++++++
 1 file changed, 19 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
index f795362f5b77e..d9e8610b5f83f 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
@@ -15,6 +15,7 @@
 
 	aliases {
 		serial0 = &uart0;
+		serial1 = &uart1;
 		ethernet0 = &emac;
 	};
 
@@ -324,6 +325,24 @@
 	status = "okay";
 };
 
+/* There's the BT part of the AP6256 connected to that UART */
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins>, <&uart1_rts_cts_pins>;
+	uart-has-rtscts;
+	status = "okay";
+
+	bluetooth {
+		compatible = "brcm,bcm4345c5";
+		clocks = <&rtc 1>;
+		clock-names = "lpo";
+		device-wakeup-gpios = <&r_pio 1 2 GPIO_ACTIVE_HIGH>; /* PM2 */
+		host-wakeup-gpios = <&r_pio 1 1 GPIO_ACTIVE_HIGH>; /* PM1 */
+		shutdown-gpios = <&r_pio 1 4 GPIO_ACTIVE_HIGH>; /* PM4 */
+		max-speed = <1500000>;
+	};
+};
+
 &usb2otg {
 	/*
 	 * This board doesn't have a controllable VBUS even though it

From c74e4ba1e28d5808cda02b34eee59dc1a5f15a6d Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Wed, 27 Mar 2019 13:43:25 +0100
Subject: [PATCH 34/34] arm64: dts: allwinner: orange-pi-3: Enable USB 3.0 host
 support

Enable Allwinner's USB 3.0 phy and the host controller. Orange Pi 3
board has GL3510 USB 3.0 4-port hub connected to the SoC's USB 3.0
port. All four ports are exposed via USB3-A connectors. The hub is
powered directly from DCIN/VCC-5V.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts | 9 +++++++++
 1 file changed, 9 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
index d9e8610b5f83f..afee79fb88f18 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
@@ -126,6 +126,10 @@
 	status = "okay";
 };
 
+&dwc3 {
+	status = "okay";
+};
+
 &ehci0 {
 	status = "okay";
 };
@@ -359,3 +363,8 @@
 	usb3_vbus-supply = <&reg_vcc5v>;
 	status = "okay";
 };
+
+&usb3phy {
+        phy-supply = <&reg_vcc5v>;
+        status = "okay";
+};
