################################################################################
# Device defaults
################################################################################

  # Additional kernel make parameters
    KERNEL_MAKE_EXTRACMD+=" overlays/slice.dtbo overlays/ws2812.dtbo"

  # NOOBS supported hex versions (legacy)
    NOOBS_HEX="2,3,4,5,6,7,8,9,d,e,f,10,11,12,14,19,0092,0093"

  # NOOBS supported model versions
    NOOBS_SUPPORTED_MODELS='"Pi Model","Pi Compute Module","Pi Zero"'

  # Additional Firmware
    FIRMWARE="${FIRMWARE} slice-firmware"

  # Additional drivers
    ADDITIONAL_DRIVERS="${ADDITIONAL_DRIVERS} slice-drivers"
