diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-one-plus.dts b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-one-plus.dts
index 12e17567ab56..fd9dcefcd223 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-one-plus.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-one-plus.dts
@@ -9,4 +9,86 @@
 / {
 	model = "OrangePi One Plus";
 	compatible = "xunlong,orangepi-one-plus", "allwinner,sun50i-h6";
+
+	aliases {
+		ethernet0 = &emac;
+	};
+
+	connector {
+		compatible = "hdmi-connector";
+		type = "a";
+		ddc-supply = <&reg_ddc>;
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
+	reg_ddc: ddc-io {
+		compatible = "regulator-fixed";
+		regulator-name = "ddc-io";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		enable-active-high;
+		gpio = <&pio 7 2 GPIO_ACTIVE_HIGH>; /* PH2 */
+	};
+
+	reg_gmac_3v3: gmac-3v3 {
+                compatible = "regulator-fixed";
+                regulator-name = "vcc-gmac-3v3";
+                regulator-min-microvolt = <3300000>;
+                regulator-max-microvolt = <3300000>;
+                startup-delay-us = <100000>;
+                enable-active-high;
+                gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>; /* PD6 */
+                vin-supply = <&reg_aldo2>;
+	};
+
+	reg_usb_vbus: vbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usb-vbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		startup-delay-us = <100000>;
+		gpio = <&r_pio 0 5 GPIO_ACTIVE_HIGH>;
+		enable-active-high;
+	};
+};
+
+&de {
+	status = "okay";
+};
+
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&ext_rgmii_pins>;
+	phy-mode = "rgmii";
+	phy-handle = <&ext_rgmii_phy>;
+	phy-supply = <&reg_gmac_3v3>;
+	allwinner,rx-delay-ps = <200>;
+	allwinner,tx-delay-ps = <200>;
+	status = "okay";
+};
+
+&gpu {
+	mali-supply = <&reg_dcdcc>;
+};
+
+&hdmi {
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
 };
