From: Szymon Janc <szymon.janc@...>
Subject: [PATCH 5/5] sixaxis: Fix multi-line comments style
Newsgroups: gmane.linux.bluez.kernel
Date: 2015-06-15 18:28:30 GMT (36 weeks, 4 days, 21 hours and 33 minutes ago)

---
 plugins/sixaxis.c | 12 ++++++++----
 1 file changed, 8 insertions(+), 4 deletions(-)

diff --git a/plugins/sixaxis.c b/plugins/sixaxis.c
index 782a89f..9b6cad4 100644
--- a/plugins/sixaxis.c
+++ b/plugins/sixaxis.c
@@ -435,9 +435,11 @@ static bool setup_device(int fd, int index, struct btd_adapter *adapter)
 	if (get_master_bdaddr(fd, &master_bdaddr) < 0)
 		return false;

-	/* This can happen if controller was plugged while already connected
+	/*
+	 * This can happen if controller was plugged while already connected
 	 * eg. to charge up battery.
-	 * Don't set LEDs in that case, hence return false */
+	 * Don't set LEDs in that case, hence return false
+	 */
 	device = btd_adapter_find_device(adapter, &device_bdaddr,
 							BDADDR_BREDR);
 	if (device && btd_device_is_connected(device))
@@ -533,8 +535,10 @@ static int get_js_number(struct udev_device *udevice)
 		if (!input_parent)
 			goto next;

-		/* check if this is the joystick relative to the hidraw device
-		 * above */
+		/*
+		 * check if this is the joystick relative to the hidraw device
+		 * above
+		 */
 		input_id = udev_device_get_sysattr_value(input_parent, "uniq");

 		/*
-- 
2.1.4

