#!/bin/sh

################################################################################
#      This file is part of OpenELEC - http://www.openelec.tv
#      Copyright (C) 2009-2014 Stephan Raue (stephan@openelec.tv)
#
#  OpenELEC is free software: you can redistribute it and/or modify
#  it under the terms of the GNU General Public License as published by
#  the Free Software Foundation, either version 2 of the License, or
#  (at your option) any later version.
#
#  OpenELEC is distributed in the hope that it will be useful,
#  but WITHOUT ANY WARRANTY; without even the implied warranty of
#  MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
#  GNU General Public License for more details.
#
#  You should have received a copy of the GNU General Public License
#  along with OpenELEC.  If not, see <http://www.gnu.org/licenses/>.
################################################################################

# setup alsa (especially the mixer config)

mixer() {
  parm=${4:-on}
  amixer -c "$1" sset "$2" "$3" $parm >/dev/null 2>&1
  amixer -c "$1" sset "$2" $parm >/dev/null 2>&1
}

(
. /etc/profile

progress "Setting up sound card"

if [ -f $HOME/.config/sound.conf ]; then

  alsactl restore -f $HOME/.config/sound.conf

else

# get card num
  card=`echo $1 | sed 's/[^0-9]*//g'`

# set common mixer params
  mixer $card Master 0db
  mixer $card Front 100%
  mixer $card PCM 0db
  mixer $card Synth 100%

# mute CD, since using digital audio instead
  mixer $card CD 0% mute

# Only unmute Line and Aux if they are possibly used.
#  mixer $card Line 100%
#  mixer $card Aux 100%

# mute mic
  mixer $card Mic 0% mute

# ESS 1969 chipset has 2 PCM channels
  mixer $card PCM,1 100%

# Trident/YMFPCI/emu10k1
  mixer $card Wave 100%
  mixer $card Music 100%
  mixer $card AC97 100%
  mixer $card Surround 90%
  mixer $card 'Surround Digital' 90%
  mixer $card 'Wave Surround' 90%
  mixer $card 'Duplicate Front' 90%
  mixer $card 'Sigmatel 4-Speaker Stereo' 90%

# CS4237B chipset:
  mixer $card 'Master Digital' 100%

# DRC
  mixer $card 'Dynamic Range Compression' 90%

# Envy24 chips with analog outs
  mixer $card DAC 100%
  mixer $card DAC,0 100%
  mixer $card DAC,1 100%

# some notebooks use headphone instead of master
  mixer $card Headphone 100%
  mixer $card Speaker 100%
  mixer $card 'Internal Speaker' 0% mute
  mixer $card Playback 100%
  mixer $card Headphone 100%
  mixer $card Speaker 100%
  mixer $card Center 100%
  mixer $card LFE 100%
  mixer $card Center/LFE 100%

# Intel P4P800-MX  (Ubuntu bug #5813)
  mixer $card 'Master Playback Switch' on

# set digital output mixer params
  mixer $card 'IEC958' 100% on
  mixer $card 'IEC958 Output' 100%
  mixer $card 'IEC958 Coaxial' 100%
  mixer $card 'IEC958 LiveDrive' 100%
  mixer $card 'IEC958 Optical Raw' 100%
  mixer $card 'SPDIF Out' 100%
  mixer $card 'SPDIF Front' 100%
  mixer $card 'SPDIF Rear' 100%
  mixer $card 'SPDIF Center/LFE' 100%
  mixer $card 'Master Digital' 100%

  mixer $card 'Analog Front' 100%
  mixer $card 'Analog Rear' 100%
  mixer $card 'Analog Center/LFE' 100%

# ASRock ION 330 (and perhaps others) has 2 IEC958 channels
  mixer $card IEC958,0 on
  mixer $card IEC958,1 on

# some ION2 has much more IEC958 channels ...
  mixer $card IEC958,2 on
  mixer $card IEC958,3 on

# ASRock ION 330 has Master Front set to 0
  mixer $card 'Master Front' 100%

# Shuttle XS35GT needs this too
  mixer $card 'Master',0 100% on

# and this for various Fusion devices like Zotac ZBOX
  mixer $card 'Front',0 100% on

# NVidia CK804 sound devices
  mixer $card 'IEC958 Playback AC97-SPSA' 100%
fi

exit 0
)&
