---
layout: page
title: "Garadget Cover"
description: "Instructions how to integrate Garadget covers within Home Assistant."
date: 2016-10-24 14:25
sidebar: true
comments: false
sharing: true
footer: true
logo: garadget.png
ha_category: Cover
ha_release: 0.32
ha_iot_class: "Cloud Polling"
---


The `garadget` cover platform lets you control [Garadget](http://www.garadget.com/) garage door futurizers through Home Assistant.

To enable Garadget Covers in your installation, add the following to your `configuration.yaml` file:

```yaml
# Example configuration.yaml entry
cover:
  - platform: garadget
    covers:
        190028001947343412342341:
          username: UseYourLogin@garadget.com
          password: abc123
      4c003f001151353432134214:
        access_token: df4cc785ff818f2b01396c44142342fccdef
```

Configuration variables:

- **covers** array (*Required*): List of your doors.
  - **device** (*Required*): This is the device id from your Garadget portal.
  - Either:
    - **username** (*Required*): Your Garadget account username.
    - **password** (*Required*): Your Garadget account password.
  - Or: 
    - **access_token** (*Required*): A generated `access_token` from your Garadget account.
  - **name** (*Optional*): Name to use in the frontend, will use name configured in Garadget otherwise.


If provided, the **access_token** will be used, otherwise the **username** and **password** will be used to automatically generate an access token at start time.


**Example with more detail:**
<p class='img'>
  <img src='{{site_root}}/images/components/garadget/cover_garadget_details.png' />
</p>

```yaml
# Related configuration.yaml entry
cover:
  - platform: garadget
    covers:
      190028001947343412342341:
        access_token: !secret garadget_access_token
        name: Garage door

sensor:
  - platform: template
    sensors:
      garage_door_status:
        friendly_name: 'State of the door'
        value_template: {% raw %}'{{ states.cover.garage_door.state }}'{% endraw %}
      garage_door_time_in_state:
        friendly_name: 'Since'
        value_template: {% raw %}'{{ states.cover.garage_door.attributes.time_in_state }}'{% endraw %}
      garage_door_wifi_signal_strength:
        friendly_name: 'WiFi strength'
        value_template: {% raw %}'{{ states.cover.garage_door.attributes.wifi_signal_strength }}'{% endraw %}
        unit_of_measurement: 'dB'

group:
  garage_door:
    name: Garage door
    entities:
      - cover.garage_door
      - sensor.garage_door_status
      - sensor.garage_door_time_in_state
      - sensor.garage_door_wifi_signal_strength

customize:
  sensor.garage_door_time_in_state:
    icon: mdi:timer-sand
  sensor.garage_door_wifi_signal_strength:
    icon: mdi:wifi
```

Some of the Garadget sensors can create a lot of clutter in the logbook.  Use this section of code in your `configuration.yaml` to exclude those entries.

```yaml
logbook:
  exclude:
    entities:
      - sensor.garage_door_time_in_state
      - sensor.garage_door_wifi_signal_strength
```

As of firmware release 1.17 the garadget device has native support for MQTT. The options allow the end-user to configure the device in the following ways 'cloud only', 'cloud and MQTT' or 'MQTT only'.

For configuration of the garadget as a MQTT cover:

```yaml
cover:
  - platform: mqtt
    name: "Garage Door"
    command_topic: "garadget/device_name/command"
    state_topic: "garadget/device_name/status"
    payload_open: "open"
    payload_close: "close"
```
