---
layout: page
title: "LimitlessLED"
description: "Instructions on how to setup LimitlessLED within Home Assistant."
date: 2015-12-03 13:00
sidebar: true
layout: page
comments: false
sharing: true
footer: true
logo: limitlessled_logo.png
ha_category: Light
ha_iot_class: "Assumed State"
ha_release: pre 0.7
---

`limitlessled` can control your LimitlessLED lights from within Home Assistant. The lights are also known as EasyBulb, AppLight, AppLamp, [MiLight](http://www.milight.com/), LEDme, dekolight, or iLight.

LimitlessLED bulbs are controlled via groups, so you can only control an individual bulb via the bridge if it is in a group by itself.

Note: you can assign an `rgbw`, `rgbww`, `white` and `dimmer` group to the same group number, effectively allowing up to 16 groups (4 `rgbww`, 4 `rgbw`, 4 `white` and 4 `dimmer`) per bridge.

An archive of the extensive API can be found [here](https://github.com/Fantasmos/LimitlessLED-DevAPI).

### {% linkable_title Setup %}

Before configuring Home Assistant, make sure you can control your bulbs or LEDs with the MiLight mobile application. Next, discover your bridge(s) IP address. You can do this via your router or a mobile application like Fing ([android](https://play.google.com/store/apps/details?id=com.overlook.android.fing&hl=en) or [iTunes](https://itunes.apple.com/us/app/fing-network-scanner/id430921107?mt=8)).

To add `limitlessled` to your installation, add the following to your `configuration.yaml` file:

```yaml
# Example configuration.yaml entry
light:
  platform: limitlessled
  bridges:
    - host: 192.168.1.10
      groups:
      - number: 1
        name: Bedroom
      - number: 2
        type: rgbw
        name: Bathroom
      - number: 3
        type: rgbw
        name: Kitchen
        fade: true
      - number: 4
        type: dimmer
        name: Livingroom
    - host: 192.168.1.11
      groups:
      - number: 1
        name: Living Room & Hall
      - number: 1
        type: bridge-led
        name: Bridge Light
```

{% configuration %}
bridges:
  description: A list of bridges.
  required: true
  type: list
  keys:
    host:
      description: IP address of the device, e.g., `192.168.1.32`.
      required: true
      type: string
    version:
      description: Bridge version.
      required: false
      default: 6
      type: integer
    port:
      description: Bridge port. For older bridges than `v6` choose `8899`.
      required: false
      default: 5987
      type: integer
    groups:
      description: The list of available groups.
      required: true
      type: list
      keys:
        number:
          description: Group number (`1`-`4`). Corresponds to the group number on the remote. These numbers may overlap only if the type is different.
          required: true
          type: integer
        name:
          description: Any name you'd like. Must be unique among all configured groups.
          required: true
          type: string
        type:
          description: Type of group. Choose either `rgbww`, `rgbw`, `white`, `bridge-led` or `dimmer`. Use `bridge-led` to control the built-in LED of newer WiFi bridges.
          required: false
          default: rgbw
          type: string
        fade:
          description: Fade behavior. If turned on (true), the group is faded out before being turned off. This makes for a more pleasing transition at the expense of wall switch usability since the light will turn back on at the lowest brightness if it is power cycled.
          required: false
          default: false
          type: boolean
{% endconfiguration %}

### {% linkable_title Night Effect %}

LimitlessLED has a `night` effect that can be used to dim the lights below `brightness: 1`. This night mode is meant to temporarily turn the lights into a nightlight. This mode can be especially helpful when wall switches are also being used. For example, when a light is using the `night` effect one way to return it to its previous brightness level (other than using Home Assistant) is to switch the lights off and then back on from the wall switch.

Note that the `brightness`, `color` and `temperature` attributes cannot be used when using the `night` effect. You can turn on `night` effect by using the `effect` attribute of the normal `light.turn_on` service. Here is an example:

```yaml
automation:
  - alias: ...
    trigger:
      # ...
    action:
      - service: light.turn_on
        data:
          entity_id: light.office, light.kitchen
          effect: night
```

### {% linkable_title Properties %}

Refer to the [light]({{site_root}}/components/light/) documentation for general property usage, but keep in mind the following notes specific to LimitlessLED.

- **RGBWW** (Only supported on v6 bridges)
  - *Color*: There are 25,856 color possibilities along the LimitlessLED color spectrum. For colors, hue and saturation can be used, but not lightness. If you select a color with lightness, Home Assistant will calculate the nearest valid LimitlessLED color. In white mode, the temperature can be set.
  - *Temperature*: There are 101 temperature steps.
  - *Brightness*: There are 101 brightness steps.
- **RGBW**
  - *Color*: There are 256 color possibilities along the LimitlessLED color spectrum. Color properties like saturation and lightness cannot be used - only Hue can. The only exception is white (which may be warm or cold depending on the type of RGBW bulb). If you select a color with saturation or lightness, Home Assistant will calculate the nearest valid LimitlessLED color.
  - *Brightness*: Wifi bridge v6 supports 101 brightness steps; older versions only 25.
- **White**
  - When using a legacy WiFi bridge (before v6), you can observe on the MiLight mobile application, you can not select a specific brightness or temperature - you can only step each property up or down. There is no indication of which step you are on. This restriction, combined with the unreliable nature of LimitlessLED transmissions, means that setting white bulb properties is done on a best-effort basis. The only very reliable settings are the minimum and maximum of each property.
  - *Temperature*: Wifi bridge v6 supports 101 temperature steps; older versions only 10.
  - *Brightness*: Wifi bridge v6 supports 101 brightness steps; older versions only 10.
- **Dimmer** (Only supported on v6 bridges)
  - This type is for a single color LED dimmer like the 1CH MiLight dimmer module or similar. This type is only supported by the version 6 Wifi bridges.
  - *Brightness*: Wifi bridge v6 supports 101 brightness steps.
- **Transitions**
  - If a transition time is set, the group will transition between the current settings and the target settings for the duration specified. Transitions from or to white are not possible - the color will change immediately.

### {% linkable_title Initialization & Synchronization %}

When starting Home Assistant, the last recorded state will be shown. This might no longer match the actual state of the bulbs.

If you control your LimitlessLED lights via the MiLight mobile application or other means while Home Assistant is running, Home Assistant cannot track those changes and you may observe obsolete information.

This lack of synchronization is due to a LimitlessLED limitation.

<p class='img'>
<img src='/images/screenshots/limitlessled_assumed_state.png' />
</p>

Because LimitlessLED lights may have an obsolete state, Home Assistant shows the power switch as two buttons rather than a toggle. This ensures that the power can be set with a single click even if the assumed state is wrong. You can change to use the power toggle with [Customize](/docs/configuration/customizing-devices/):

```yaml
homeassistant:
  customize_domain:
    light:
      assumed_state: false
```
