---
layout: page
title: "Tomato"
description: "Instructions on how to integrate Tomato routers into Home Assistant."
date: 2015-03-23 19:59
sidebar: true
comments: false
sharing: true
footer: true
logo: tomato.png
ha_category: Presence Detection
ha_release: pre 0.7
---

The `tomato` platform requires an extra config variable called `http_id`. The
value can be obtained by logging in to the Tomato admin interface and search for
`http_id` in the page source code.

Because of a limitation in Tomato's API, this platform will only track wireless devices.
If tracking wired devices like a Philips Hue Hub is necessary,
it is possible to use another platform like [Nmap](/components/device_tracker.nmap_tracker/).

To use this device tracker in your installation,
add the following to your `configuration.yaml` file:

```yaml
# Example configuration.yaml entry
device_tracker:
  - platform: tomato
    host: YOUR_ROUTER_IP_ADDRESS
    username: YOUR_ADMIN_USERNAME
    password:  YOUR_ADMIN_PASSWORD
    http_id: YOUR_HTTP_ID
```

{% configuration %}
host:
  description: "The IP address or hostname of your router, e.g., `192.168.1.1` or `rt-ac68u`."
  required: true
  type: string
port:
  description: "The port number of your router, e.g., `443`."
  required: false
  type: integer
  default: 80/443 (automatically detected)
ssl:
  description: "Whether to connect via `https`."
  required: false
  type: boolean
  default: false
verify_ssl:
  description: "If SSL verification for https resources needs to be turned off (for self-signed certs, etc.) this can take on boolean values `False` or `True` or you can pass a location on the device where a certificate can be used for verification e.g., `/mnt/NAS/router_cert.pem`."
  required: false
  type: [string, boolean]
  default: true
username:
  description: "The username of an user with administrative privileges, usually *admin*."
  required: true
  type: string
password:
  description: "The password for your given admin account."
  required: true
  type: string
http_id:
  description: "The value can be obtained by logging in to the Tomato admin interface and search for `http_id` in the page source code."
  required: true
  type: string
{% endconfiguration %}

See the [device tracker component page](/components/device_tracker/) for
instructions how to configure the people to be tracked.

A description of the API s available in this
[Tomato API](http://paulusschoutsen.nl/blog/2013/10/tomato-api-documentation/)
blog post.

SSL Certificate:

Gathering the SSL Certificate of your router can be accomplished with this (or
a similar) command:
```bash
openssl s_client -showcerts -connect 172.10.10.1:443 </dev/null 2>/dev/null | openssl x509 -outform PEM > router_cert.pem
```
