console=tty1
selinux=permissive
enforcing=0
optargs=no_console_suspend panic=10 quiet loglevel=1 ipv6.disable=1
kernel_filename=kernel.img
#initrd_filename=ramdisk.img
#recovery_initrd_filename=ramdisk-recovery.img
hardware=sun50iw1p1

# INFO:
# To enable one of below options,
# uncomment them by removing # in front of name

# To use android recovery:
# Create empty file recovery.txt in root of this partition

# To enable LCD or HDMI, if not changed it will use default (experimental)
disp_screen0=hdmi
# disp_screen1=lcd or hdmi
# disp_mode=screen0 or screen1 or dualhead or xinerama or clone

# USB OTG port mode (experimental)
# otg_mode=device or host or otg
otg_mode=host

# Configure contiguous memory allocation
# This maybe required to be enlarged for 4K displays
cma=384M

# To change HDMI display mode:
# hdmi_mode=480i
# hdmi_mode=576i
# hdmi_mode=480p
# hdmi_mode=576p
# hdmi_mode=720p50
hdmi_mode=720p60
# hdmi_mode=1080i50
# hdmi_mode=1080i60
# hdmi_mode=1080p24
# hdmi_mode=1080p50
# hdmi_mode=1080p60
# hdmi_mode=2160p30
# hdmi_mode=2160p25
# hdmi_mode=2160p24

# To enable DVI compatibilty:
disp_dvi_compat=on

# To enable CSI camera, if not enabled it will use default:
# camera_type=s5k4ec
# camera_type=ov5640

# Configure ethernet speed
eth0_speed=auto
# eth0_speed=1000
# eth0_speed=100
# eth0_speed=10

# Disable HDMI CEC
hdmi_cec=0

# Enable experimental HDMI CEC driver
# hdmi_cec=2
