(module Connectors_Terminal_Blocks:TerminalBlock_bornier-2_P5.08mm (layer F.Cu) (tedit 59FF03AB)
  (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
  (tags "terminal block bornier2")
  (fp_text reference J1 (at 2.54 -5.08) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "Screw Term." (at 2.54 5.08) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 7.79 4) (end -2.71 4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.79 4) (end 7.79 -4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.71 -4) (end -2.71 4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.71 -4) (end 7.79 -4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.54 3.81) (end 7.62 3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.54 -3.81) (end -2.54 3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.62 -3.81) (end -2.54 -3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.62 3.81) (end 7.62 -3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.62 2.54) (end -2.54 2.54) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.54 -3.75) (end -2.46 -3.75) (layer F.Fab) (width 0.1))
  (fp_line (start 7.54 3.75) (end 7.54 -3.75) (layer F.Fab) (width 0.1))
  (fp_line (start -2.46 3.75) (end 7.54 3.75) (layer F.Fab) (width 0.1))
  (fp_line (start -2.46 -3.75) (end -2.46 3.75) (layer F.Fab) (width 0.1))
  (fp_line (start -2.41 2.55) (end 7.49 2.55) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 2.54 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 2 thru_hole circle (at 5.08 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask))
  (model Connectors_Phoenix.3dshapes/PhoenixContact_MCV-G_02x5.08mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
