---
layout: page
title: "Xiaomi Binary Sensor"
description: "Instructions on how to setup the Xiaomi binary sensors within Home Assistant."
date: 2017-07-21 16:34
sidebar: true
comments: false
sharing: true
footer: true
logo: xiaomi.png
ha_category: Binary Sensor
ha_release: "0.50"
ha_iot_class: "Local Push"
---

The `xiaomi aqara` binary sensor platform allows you to get data from your [Xiaomi](http://www.mi.com/en/) binary sensors.

The requirement is that you have setup the [`xiaomi aqara` component](/components/xiaomi_aqara/).

### {% linkable_title Type of sensors supported %}

| Name | Zigbee entity | Model no. | States | Event | Event key | Event values |
| ---- | ------------- | --------- | ------ | ----- | --------- | ------------ |
| Motion Sensor (1st gen) | motion | RTCGQ01LM | on, off | `motion` | | |
| Motion Sensor (2nd gen) | sensor_motion.aq2 | RTCGQ11LM | on, off | `motion` | | |
| Door and Window Sensor (1st gen) | magnet | WSDCGQ01LM | on, off | | | |
| Door and Window Sensor (2nd gen) | sensor_magnet.aq2 | MCCGQ11LM | on, off | | | |
| Smoke Detector | smoke | JTYJ-GD-01LM/BW | on, off | | | |
| Gas Leak Detector | natgas | JTQJ-BF-01LM/BW | on, off | | | |
| Water Leak Sensor | sensor_wleak.aq1 | SJCGQ11LM | on, off | | | |
| Button (1st gen) | switch | WXKG01LM | on (through long_click_press), off | `click`| `click_type`| `long_click_press`, `long_click_release`, `hold`, `single`, `double` |
| Button (2nd gen) | sensor_switch.aq2, remote.b1acn01 | WXKG11LM | off (always) | `click` | `click_type` | `single`, `double` |
| Aqara Wireless Switch (Single) | 86sw1 | WXKG03LM | off (always) | `click` | `click_type` | `single` |
| Aqara Wireless Switch (Double) | 86sw2 | WXKG02LM | off (always) | `click` | `click_type` | `single`, `both` |
| Cube | cube | MFKZQ01LM | off (always) | `cube_action` | `action_type`, `action_value` (rotate) | `flip90`, `flip180`, `move`, `tap_twice`, `shake_air`, `swing`, `alert`, `free_fall`, `rotate` (degrees at action_value) |
| Vibration Sensor | vibration | DJT11LM | off (always) | `xiaomi_aqara.movement` | `movement_type` | `vibrate`, `tilt`, `free_fall` |

### {% linkable_title Automation examples %}

#### {% linkable_title Motion %}

```yaml
- alias: If there is motion and its dark turn on the gateway light
  trigger:
    platform: state
    entity_id: binary_sensor.motion_sensor_158d000xxxxxc2
    from: 'off'
    to: 'on'
  condition:
    condition: numeric_state
    entity_id: sensor.illumination_34ce00xxxx11
    below: 300
  action:
    - service: light.turn_on
      entity_id: light.gateway_light_34ce00xxxx11
      data:
        brightness: 5
    - service: automation.turn_on
      data:
        entity_id: automation.MOTION_OFF
- alias: If there no motion for 5 minutes turn off the gateway light
  trigger:
    platform: state
    entity_id: binary_sensor.motion_sensor_158d000xxxxxc2
    from: 'on'
    to: 'off'
    for:
      minutes: 5
  action:
    - service: light.turn_off
      entity_id: light.gateway_light_34ce00xxxx11
    - service: automation.turn_off
      data:
        entity_id: automation.Motion_off
```

#### {% linkable_title Door and/or Window %}

```yaml
- alias: If the window is open turn off the radiator
  trigger:
    platform: state
    entity_id: binary_sensor.door_window_sensor_158d000xxxxxc2
    from: 'off'
    to: 'on'
  action:
    service: climate.set_operation_mode
    entity_id: climate.livingroom
    data:
      operation_mode: 'Off'
- alias: If the window is closed for 5 minutes turn on the radiator again
  trigger:
    platform: state
    entity_id: binary_sensor.door_window_sensor_158d000xxxxxc2
    from: 'on'
    to: 'off'
    for:
      minutes: 5
  action:
    service: climate.set_operation_mode
    entity_id: climate.livingroom
    data:
      operation_mode: 'Smart schedule'
```

#### {% linkable_title Smoke %}

```yaml
- alias: Send notification on fire alarm
  trigger:
    platform: state
    entity_id: binary_sensor.smoke_sensor_158d0001574899
    from: 'off'
    to: 'on'
  action:
    - service: notify.html5
      data:
        title: Fire alarm!
        message: Fire/Smoke detected!
    - service: xiaomi_aqara.play_ringtone
      data:
        gw_mac: xxxxxxxxxxxx
        ringtone_id: 2
        ringtone_vol: 100
```

#### {% linkable_title Gas %}

```yaml
- alias: Send notification on gas alarm
  trigger:
    platform: state
    entity_id: binary_sensor.natgas_sensor_158dxxxxxxxxxx
    from: 'off'
    to: 'on'
  action:
    - service: notify.html5
      data_template:
        title: Gas alarm!
        message: 'Gas with a density of {% raw %}{{ states.binary_sensor.natgas_sensor_158dxxxxxxxxxx.attributes.density }}{% endraw %} detected.'
```

#### {% linkable_title Xiaomi Wireless Button %}

Available events are `single`, `double`, `hold`, `long_click_press` and `long_click_release`. For Square version (Aqara brand) only `single` and `double` events are supported. Furthermore the space between two clicks to generate a double click must be quite large now.

```yaml
- alias: Toggle dining light on single press
  trigger:
    platform: event
    event_type: click
    event_data:
      entity_id: binary_sensor.switch_158d000xxxxxc2
      click_type: single
  action:
    service: switch.toggle
    entity_id: switch.wall_switch_left_158d000xxxxx01
- alias: Toggle couch light on double click
  trigger:
    platform: event
    event_type: click
    event_data:
      entity_id: binary_sensor.switch_158d000xxxxxc2
      click_type: double
  action:
    service: switch.toggle
    entity_id: switch.wall_switch_right_158d000xxxxx01
- alias: Let a dog bark on long press
  trigger:
    platform: event
    event_type: click
    event_data:
      entity_id: binary_sensor.switch_158d000xxxxxc2
      click_type: long_click_press
  action:
    service: xiaomi_aqara.play_ringtone
    data:
      gw_mac: xxxxxxxxxxxx
      ringtone_id: 8
      ringtone_vol: 8
```

#### {% linkable_title Xiaomi Cube %}

Available events are `flip90`, `flip180`, `move`, `tap_twice`, `shake_air`, `swing`, `alert`, `free_fall` and `rotate`. The component stores the last action as the attribute `last_action`.

```yaml
- alias: Cube event flip90
  trigger:
    platform: event
    event_type: cube_action
    event_data:
      entity_id: binary_sensor.cube_15xxxxxxxxxxxx
      action_type: flip90
  action:
    - service: light.turn_on
      entity_id: light.gateway_light_28xxxxxxxxxx
      data:
        color_name: "springgreen"
- alias: Cube event flip180
  trigger:
    platform: event
    event_type: cube_action
    event_data:
      entity_id: binary_sensor.cube_15xxxxxxxxxxxx
      action_type: flip180
  action:
    - service: light.turn_on
      entity_id: light.gateway_light_28xxxxxxxxxx
      data:
        color_name: "darkviolet"
- alias: Cube event move
  trigger:
    platform: event
    event_type: cube_action
    event_data:
      entity_id: binary_sensor.cube_15xxxxxxxxxxxx
      action_type: move
  action:
    - service: light.turn_on
      entity_id: light.gateway_light_28xxxxxxxxxx
      data:
        color_name: "gold"
- alias: Cube event tap_twice
  trigger:
    platform: event
    event_type: cube_action
    event_data:
      entity_id: binary_sensor.cube_15xxxxxxxxxxxx
      action_type: tap_twice
  action:
    - service: light.turn_on
      entity_id: light.gateway_light_28xxxxxxxxxx
      data:
        color_name: "deepskyblue"
- alias: Cube event shake_air
  trigger:
    platform: event
    event_type: cube_action
    event_data:
      entity_id: binary_sensor.cube_15xxxxxxxxxxxx
      action_type: shake_air
  action:
    - service: light.turn_on
      entity_id: light.gateway_light_28xxxxxxxxxx
      data:
        color_name: "blue"
```

#### {% linkable_title Aqara Wireless Switch %}

The Aqara Wireless Switch is available as single-key and double-key version. Each key behaves like the Wireless Button limited to the click event `single`. The double key version adds a third device called `binary_sensor.wall_switch_both_158xxxxxxxxx12` which reports a click event called `both` if both keys are pressed.

```yaml
- alias: Decrease brightness of the gateway light
  trigger:
    platform: event
    event_type: click
    event_data:
      entity_id: binary_sensor.wall_switch_left_158xxxxxxxxx12
      click_type: single
  action:
    service: light.turn_on
    entity_id: light.gateway_light_34xxxxxxxx13
    data_template:
      brightness: {% raw %}>-
        {% if states.light.gateway_light_34xxxxxxxx13.attributes.brightness %}
          {% if states.light.gateway_light_34xxxxxxxx13.attributes.brightness - 60 >= 10 %}
            {{states.light.gateway_light_34xxxxxxxx13.attributes.brightness - 60}}
          {% else %}
            {{states.light.gateway_light_34xxxxxxxx13.attributes.brightness}}
          {% endif %}
        {% else %}
          10
        {% endif %}{% endraw %}

- alias: Increase brightness of the gateway light
  trigger:
    platform: event
    event_type: click
    event_data:
      entity_id: binary_sensor.wall_switch_right_158xxxxxxxxx12
      click_type: single
  action:
    service: light.turn_on
    entity_id: light.gateway_light_34xxxxxxxx13
    data_template:
      brightness: {% raw %}>-
        {% if states.light.gateway_light_34xxxxxxxx13.attributes.brightness %}
          {% if states.light.gateway_light_34xxxxxxxx13.attributes.brightness + 60 <= 255 %}
            {{states.light.gateway_light_34xxxxxxxx13.attributes.brightness + 60}}
          {% else %}
            {{states.light.gateway_light_34xxxxxxxx13.attributes.brightness}}
          {% endif %}
        {% else %}
          10
        {% endif %}{% endraw %}

- alias: Turn off the gateway light
  trigger:
    platform: event
    event_type: click
    event_data:
      entity_id: binary_sensor.wall_switch_both_158xxxxxxxxx12
      click_type: both
  action:
    service: light.turn_off
    entity_id: light.gateway_light_34xxxxxxxx13
```

#### {% linkable_title Vibration Sensor %}

This automation toggles the living room lamp on vibration/tilt.

```yaml
- alias: Turn on Living Room Lamp on vibration
  trigger:
    platform: event
    event_type: xiaomi_aqara.movement
    event_data:
      entity_id: binary_sensor.vibration_xxxx000000
      movement_type: vibrate
  action:
    service: light.toggle
    data:
      entity_id: light.living_room_lamp
- alias: Turn on Living Room Lamp on tilt
  trigger:
    platform: event
    event_type: xiaomi_aqara.movement
    event_data:
      entity_id: binary_sensor.vibration_xxxx000000
      movement_type: tilt
  action:
    service: light.toggle
    data:
      entity_id: light.living_room_lamp
```
